{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["1-产业分类","2-透视","3-技术需求库-打印"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"1-产业分类","index":0,"n_rows":15,"n_cols":2,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
["编号","产业分类"]
[{"$f":"ROW()-2","v":1},"汽车电子及新型汽车零部件"]
[{"$f":"ROW()-2","v":2},"农产品加工及绿色食品"]
[3,"生物医药及先进医疗器械"]
[4,"车规级芯片及功率半导体器件"]
[5,"生物基新材料"]
[6,"碳纤维及复合材料"]
[7,"精细化工及天然气化工"]
[8,"精密仪器及先进装备"]
[9,"光电子及智能传感器"]
[10,"人工智能机智能机器人"]
[11,"新能源及动力电池"]
[12,"遥感卫星及航天航空技术"]
[13,"其他"]

{"sheet":"2-透视","index":1,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["需求产业分类","(多项)"]
[]
["行标签","计数项:企业名称"]
["长春",139]
["通化",23]
["吉林",23]
["白城",15]
["四平",13]
["白山",10]
["辽源",10]
["延边州",7]
["总计",240]

{"sheet":"3-技术需求库-打印","index":2,"n_rows":246,"n_cols":16,"rows_kept":246,"cut":false,"hidden":false,"merged":[[0,2,0,12]]}
[" "," ","吉林省工业技术研究院技术需求库",{"$nulls":10}," "," "," "]
[" "," ","序号","需求产业分类","需求领域","城市","区县","企业名称","技术需求名称","企业简况","待解决问题","企业需求","年份","月份","联系人","电话"]
[" "," ",{"$f":"ROW()-2","v":1},"精密仪器及先进装备","装备制造","长春","朝阳区","长春三友汽车部件制造有限公司"," "," "," ","铝焊接质量的稳定性。  1.智能制造电气自动化领域的电气工程师1名，能够进行电气原理图设计、电气元件的安装及接线，PLC机器人编程及调试，完善相关电气文件，及设备升级改造。  2.焊接技师2名，能够进行现场参数调整、夹具调整，机器人编程、设备故障处理及解决生产中的技术问题。  实习大学生15名，机电一体化技术、数控技术与应用、机械设计制造及其自动化或其它相关专业均可。",2018," ","孙晨玲",15124329218]
[" "," ",2,"精密仪器及先进装备","新能源","长春","朝阳区","吉林东光奥威汽车制动系统有限公司"," "," "," ","轮毂电机驱动电动汽车系列关键技术；汽车智能驻车制动及多种新型电子驻车制动器；电动智能车平台；模块化的制造执行系统；电动汽车用电机控制器；高柔性拉伸成型机；",2018," ","马志国\n张延军\n袁亮  ","17386820553\n13578763990\n13844094709"]
[" "," ",3,"碳纤维及复合材料","新材料","长春","绿园区","长春城际轨道客车配件有限公司"," "," "," ","技术难点：采用新材料、新技术代替当前的现有材料:  技术指标：超塑技术，绿色环保材料；重量轻，有韧性。  需要掌握超塑技术方面的人才；",2018," "," "," "]
[" "," ",4,"精细化工及天然气化工","石油化工","四平","双辽","双辽昊华化工有限公司"," "," "," ","以氯气为原料的精细化工产品成套生产技术，如三氯化磷、磷酸三乙酯、四氯苯醌、氯乙酸及水处理剂等。  所要达到的技术指标满足工艺包深度要求的以下产品的成套生产技术：12万吨/年三氯化磷；5万吨/年磷酸三乙酯；5kt/年四氯苯醌；5万吨/年氯乙酸及3万吨/年水处理剂；  工艺包深度要求参照中石化《石油化工装置工艺设计包（成套技术工艺包）内容规定》SHSG-052-2003。  有上述同类产品研发、设计或生产管理经验的技术人才和管理人才。  有5年以上生产管理或研发经验者优先考虑。需求数量10-20人。",2018," "," "," "]
[" "," ",5,"生物医药及先进医疗器械","生物医药医疗","通化","通化","吉林省正和药业集团股份有限公司"," "," "," ","人参须根组织培养中提高人参总皂苷含量、接骨片质量标准改进与提升开发资金。   需要医药专业大专及以上学历人员若干名。",2018," "," "," "]
[" "," ",6,"生物医药及先进医疗器械","生物医药医疗","通化","通化","通化昌源医药科技有限公司"," "," "," ","公司现需要对复春散水凝胶制剂工艺研究；复春散水凝胶技术指标检测：包括质量标准的制定、制剂稳定性考察、制剂理化性质、生化制备考察等；复春散水凝胶功效学及安全性考察：考察该制剂对烧烫伤模型、褥疮模型动物的治疗作用；考察该制剂的皮肤用药安全性；提供专利并为后期企业产品申报过程中的相关技术问题提供技术指导。  研发经费20万，可根据实施情况再研究。   中药及外用制剂研发相关人才；中药质量管理相关人员。需求8人",2018," "," "," "]
[" "," ",7,"生物医药及先进医疗器械","生物医药医疗","长春","九台区","长春呈实健康实业有限公司"," "," "," ","动脉粥样硬化早期诊断；富硒芝茸肽；新型拔牙创填充材料的开发；",2018," "," "," "]
[" "," ",8,"生物医药及先进医疗器械","生物医药医疗","长春","朝阳区","吉林省蒲川生物医药有限公司"," "," "," ","甲状腺微小癌高灵敏度基因分析芯片及检测试剂盒的研制",2018," "," "," "]
[" "," ",9,"生物医药及先进医疗器械","生物医药医疗","吉林","磐石","吉林英联生物制药股份有限公司"," "," "," ","我公司前列腺素E1采用的是从羊精囊中提取的天然酶，作为合成酶应用。由于天然酶的提取受到动物源量的限制，存在提取酶的收率、活性等不稳定，影响合成工艺收率等问题。  随着基因重组等现代生物技术的发展，利用转基因技术人工合成蛋白、生物酶后，已经得到工业化应用。为此，公司计划利用基因重组的方式，选择合适的载体表达并提取前列腺素E1合成酶，替代天然酶。可提供项目研发资金10万元。  化学合成、生物工程方面的技术人员",2018," "," "," "]
[" "," ",10,"其他","轻工纺织","辽源","辽源","辽源市优品内衣有限公司"," "," "," ","需要解决服装服饰技术研发、原材料功能技术、成衣设计等技术问题  拟可提供项目研发资金不限。   需要技术研发、原材料、以及成衣设计等技术人才。",2018," "," "," "]
[" "," ",11,"其他","轻工纺织","长春","宽城区","长春圣威雅特服装集团有限公司"," "," "," ","服装智能化生产技术需要完善和发展，争取服装智能化生产并使服装质量和数量都跃上一个新台阶。  公司亟需各类服装技术人员，丰富壮大技术中心力量，为公司服装研发提供充足动力。",2018," "," "," "]
[" "," ",12,"其他","轻工纺织","辽源","辽源","吉林省东北袜业园织袜有限公司"," "," "," ","1.技术难点：袜品的研发打样，需与国际市场同步；  2.技术指标：通过研发，达到市场占有率40%；  3.技术开发、创新项目可申请研发资金。  产品研发人才2人。",2018," "," "," "]
[" "," ",13,"农产品加工及绿色食品","农产品加工","白山","白山","大山合集团白山现代农业公司"," "," "," ","食用菌代餐粉：利用食用菌、五谷杂粮、豆类，蔬菜水果等为主要原料，开发营养全面的冲调代餐食品，要求温水快速冲调，口感细腻，香味自然。 ",2018," "," "," "]
[" "," ",14,"农产品加工及绿色食品","农产品加工","白山","白山","白山市林源春生态科技股份有限公司"," "," "," ","护眼功能产品生产工艺产品规模性生产，并销售到市场。",2018," "," "," "]
[" "," ",15,"农产品加工及绿色食品","农产品加工","通化","集安","吉林长青参业有限公司"," "," "," ","人参皂苷单体分离。在人参中包括30多种皂苷成分，是人参中的主要成分，近几年人参皂苷在治疗癌症方面起了很重大的作用，它可以很好的诱导癌细胞死亡，增强癌症患者的身体抵抗力，可以放化疗时同时使用，更好的保护免疫器官，减轻放化疗的副作用，而且人参皂苷还具有抗衰老，抗疲劳，活化皮肤细胞，增加皮肤弹性等功能。  有效的分离人参皂苷单体，可以更有效地针对市场需求。人参皂苷脱农残技术。目前我公司人参皂苷脱农残技术属于研发阶段，急需技术支持。",2018," "," "," "]
[" "," ",16,"农产品加工及绿色食品","农产品加工","通化","通化","通化力神保健品有限公司"," "," "," ","1.人参发酵、提纯技术。  2.人参深加工技术。  3.人参单体成分应用技术。  4.保健食品研发。  食品、保健品、中药研发人员：5人食品、保健品、医疗器械生产技术人员：5人。",2018," "," "," "]
[" "," ",17,"农产品加工及绿色食品","农产品加工","辽源","辽源","辽源市禹然农业发展有限公司"," "," "," ","拟投入35万专项研发资金，蒲公英茶功能饮料研发。  食品类饮料研发技术专家、蒲公英种植技术专业人才",2018," "," "," "]
[" "," ",18,"精密仪器及先进装备","电子信息","四平","四平","吉林省康达农业机械有限公司"," "," "," ","高速播种、信息化平台建设目标：播种速度达到20公里/小时；数据采集、数据传输、数据展示、数据监控、大数据平台。   机械设计制造专业本科及以上3人；  农艺专业本科及以上2人；  网络信息专业本科及以上1人。",2018," "," "," "]
[" "," ",19,"光电子及智能传感器","电子信息","吉林","吉林","吉林大仝数码科技股份有限公司"," "," "," ","需要开发建设区块链追溯系统，通过区块链追溯系统鉴别大米的产区和品种，拟投入资金120万元。  需求调研设计员1名；架构师1名。",2018," "," "," "]
[" "," ",20,"光电子及智能传感器","电子信息","吉林","吉林","吉林省通卡支付股份有限公司"," "," "," ","手机二维码支付的多票制解决方式及换乘优惠的实现方式。  NFC手机支付的交易速度、感应距离及不同型号手机的兼容性问题。   手机端系统开发人员：安卓系统开发人员，IOS系统开发人员：10名  ORACLE数据库运维人员：3名；  网路安全、系统软硬件维护人员：10名；  系统架构师：2名。",2018," "," "," "]
[" "," ",21,"精密仪器及先进装备","装备制造","长春","朝阳区","吉林省中科汽车零部件有限公司"," "," "," ","汽车电子和汽车前大灯电子研发。  汽车及零部件专业，各层次人才均可，数量按实际情况决定。",2019," "," "," "]
[" "," ",22,"精密仪器及先进装备","装备制造","吉林","吉林","吉林市吉隆科技开发有限责任公司"," "," "," ","食用菌智能装备及生产线的研制。  锅炉设计专业人才2名，非标机械设计专业人才3名，人工智能专业人才2名，软件开发人才2名。",2019," "," "," "]
[" "," ",23,"精密仪器及先进装备","装备制造","长春","二道区","长春合心机械制造有限公司"," "," "," ","智能化生产线模拟仿真及异地信息共享项目。  由于企业规模增大，现急需机械、电气方面的科技人才。",2019," "," "," "]
[" "," ",24,"精密仪器及先进装备","装备制造","长春","朝阳区","长春凯迪汽车车身设计有限公司"," "," "," ","轿车内饰复杂曲面结构数字化设计。   高质量的应届毕业生。",2019," "," "," "]
[" "," ",25,"精密仪器及先进装备","装备制造","四平","四平","四平博尓特工艺装备有限公司"," "," "," ","解决以往的硬质合金刀具在加工玻璃纤维增强塑料、填硅材料、硬质炭纤维等复合材料过程中出现的打滑、不下屑，切削温度高等不足之处。超硬刀具材料制造及工艺成果加工切削速度可达120m/min,寿命可达10m。在生产效率方面，加工效率提高1倍；在刀具消耗价格方面，刀具成本降低20%。试制出2-3种金刚石超硬刀具和立方氮化硼超硬刀具，实现相关产品小规模推广，如果量产，实现年产值1000万元，净利润35%以上。拟可提供的项目研发资金100万元。   高精密机械加工领域，涉及到的刀具材料优化选择及其应用的专业人才，研究生及其以上。",2019," "," "," "]
[" "," ",26,"精密仪器及先进装备","装备制造","四平","四平","吉林省艾斯克机电股份有限公司"," "," "," ","鸭自动掏膛生产线：家禽自动化分割设备和分割机器人，工作能力：13500只鸡/小时，或7000只鸡/小时。   大学本科机械设计、电气设计、电气自动化毕业生及有相关工作经验人员。",2019," "," "," "]
[" "," ",27,"精密仪器及先进装备","装备制造","四平","四平","四平美联热工设备制造有限公司"," "," "," ","高分子材料在特殊工况领域的应用。  高分子新材料专业专家。",2019," "," "," "]
[" "," ",28,"精密仪器及先进装备","装备制造","四平","四平","四平市巨元瀚洋板式换热器有限公司"," "," "," ","换热机组控制系统集成开发。  电气工程、暖通、自动化专业等10人。",2019," "," "," "]
[" "," ",29,"精密仪器及先进装备","装备制造","通化","通化","通化石油化工机械制造有限责任公司"," "," "," ","石油钻修井机井口自动化技术，远程数据及故障诊断、控制技术。  高端装备制造人才，信息化专业人才等具有独立设计能力的创新型人才，以及对口专业大学本科以上人才。",2019," "," "," "]
[" "," ",30,"精密仪器及先进装备","装备制造","吉林","蛟河","蛟河市守庆新能源有限责任公司"," "," "," ","生物质锅炉高效除尘换热一体化装置。  热能与动力工程，本科及以上，5名；机械设计制造及其自动化，本科及以上，3名；电气自动化，本科及以上，2名；工程造价，本科及以上，2名。",2019," "," "," "]
[" "," ",31,"精密仪器及先进装备","装备制造","长春","九台区","吉林省金博精工科技有限公司"," "," "," ","1.高速运动过程控制的算法研究。金属材料的加工特性和在使用中的力学性能分析计算。  2.气体浓度检测的实时性研究。国外自动化领域的先进技术（设备、方法、解决方案）发展情况。",2019," "," "," "]
[" "," ",32,"精密仪器及先进装备","装备制造","长春","九台区","吉林省富恒粮食收储有限公司"," "," "," ","烘干机燃煤改生物质  1、企业成本增加。经了解，改燃后烘干成本提升，烘干粮食费用每吨提高约20～40元，小型企业改造后成本难以负担。  2、烘干效率降低。改燃后生物质燃烧升温慢，生产过程中，烘干塔供热温度不均衡，导致烘干粮水分不均，烘干效率降低，日产量仅为原来的80%左右，达不到设计产能，粮食质量不稳定。  3、设备容易出现故障。由于锅炉改造均处于实验阶段，无成功经验可借鉴，改燃技术不够成熟，出现燃烧材料炼焦，堵塞烟道，生物质成本过高等问题。",2019," "," "," "]
[" "," ",33,"精密仪器及先进装备","装备制造","长春","九台区","吉林省成刚粮食收储有限公司"," "," "," ","烘干机燃煤改生物质。",2019," "," "," "]
[" "," ",34,"精密仪器及先进装备","装备制造","长春","九台区","长春市鸿森粮食收储有限公司"," "," "," ","烘干机燃煤改生物质。",2019," "," "," "]
[" "," ",35,"精密仪器及先进装备","装备制造","长春","九台区","长春明大科技发展有限公司"," "," "," ","在汽车模具设计加工制造上要提高技术设计与制造能力。  缺少汽车冲压模具技术人才，如模具设计，生产工艺管理；缺少汽车冲压模具的技术工人，如数控加工，模具钳工。",2019," "," "," "]
[" "," ",36,"碳纤维及复合材料","新材料","吉林","吉林","吉林乾仁新材料有限公司"," "," "," ","高性能碳纤维助剂的研发与应用  有机化学博士、硕士5人",2019," "," "," "]
[" "," ",37,"精细化工及天然气化工","石油化工","通化","梅河口","吉林森工化工有限责任公司"," "," "," ","1.低甲醛释放木材胶粘剂工艺技术研发与提升  2.与高等院校产学研协作  3.建立吉林省校企联合技术创新实验室   公司需要高端技术人才的加盟及高等院校的产学研协作。",2019," "," "," "]
[" "," ",38,"精细化工及天然气化工","石油化工","长春","公主岭市","吉林省八达农药有限公司"," "," "," ","1.大豆田倒茬种小麦、玉米、高粱，解决豆田除草剂残留影响问题。  2.高粱田安全、高效除草剂开发：开发出一种用于高粱田除草的除草剂。  植保、化工领域。研究生以上学历或在相关领域工作10年以上。",2019," "," "," "]
[" "," ",39,"生物医药及先进医疗器械","生物医药医疗","长春","朝阳区","吉林省太阳鸟再生医学工程有限责任公司"," "," "," ","用于重大疾病治疗的干细胞制剂研发  需要引进医学和生物学领域，具有硕士以上学位的专业人才8名。",2019," "," "," "]
[" "," ",40,"生物医药及先进医疗器械","生物医药医疗","长春","双阳区","长春世鹿鹿业集团有限公司"," "," "," ","以梅花鹿皮为原料的胶原肽系列产品开发用  食品专业本科生2名，中药学专业本科生3名",2019," "," "," "]
[" "," ",41,"生物医药及先进医疗器械","生物医药医疗","长春","朝阳区","长春生物制品研究所有限责任公司"," "," "," ","1.病毒样颗粒疫苗的研发；  2.新型佐剂疫苗；  3.大肠杆菌表达重组蛋白产品（一类创新药或首仿药）；  4.肿瘤、传染病等疾病快速床旁诊断试剂  需要病毒性疫苗、佐剂研究、重组蛋白药物、快速诊断试剂方面领军人才各  1人，为博士水平或研究员，有特殊才能可放宽要求；相关本科或硕士生各2人。",2019," "," "," "]
[" "," ",42,"生物医药及先进医疗器械","生物医药医疗","长春","德惠市","吉林省都邦药业股份有限公司"," "," "," ","生产车间智能制造改造技术需求  医药相关本科及以上相关技术人员",2019," "," "," "]
[" "," ",43,"生物医药及先进医疗器械","生物医药医疗","吉林","桦甸","吉林省红石林业局森林特色食品加工厂"," "," "," ","灵芝及灵芝孢子粉系列产品研发，产品设计、技术攻关；企业策划、市场营销、产业升级、产业融合等需求。   灵芝及灵芝孢子粉产品研发、产品设计、技术攻关、产品检验；企业策划、市场营销等方面人才。",2019," "," "," "]
[" "," ",44,"生物医药及先进医疗器械","生物医药医疗","吉林","桦甸","吉林上海胡庆余堂药业有限公司"," "," "," ","中药及保健食品的研发   药学相关专业、药品检验相关专业",2019," "," "," "]
[" "," ",45,"生物医药及先进医疗器械","生物医药医疗","四平","四平","吉林吉春制药股份有限公司"," "," "," ","驴胶补血丸、益康胶囊生产工艺研究  药品、保健食品研发领域，高层次人才，5人；要求：  1.药学、中药学、食品学及相关专业，本科以上学历；  2.熟练药品、保健食品检验操作，GMP管理、药品注册法规，善于学习，对工作认真负责。  3.负责根据新产品研发计划，开展各项药品、保健食品的研发工作，同时负责已上市产品的持续技术改进及质量标准提升工作。",2019," "," "," "]
[" "," ",46,"生物医药及先进医疗器械","生物医药医疗","白城","大安","生命肽美(吉林)生物科技股份有限公司"," "," "," ","小分子肽的肽类产品开发及技术成果转化   生物技术方面的专业人才",2019," "," "," "]
[" "," ",47,"生物医药及先进医疗器械","生物医药医疗","通化","通化","通化海恩达高科技股份有限公司"," "," "," ","无线通讯控制   技术人员缺乏中西医结合型人才，要求专业领域是医学、中医学及中西医结合",2019," "," "," "]
[" "," ",48,"生物医药及先进医疗器械","生物医药医疗","通化","梅河口","吉林丰生制药有限公司"," "," "," ","脾多肽注射液基础物质组分的确定研究   企业积极吸纳药学相关专业本科以上学历，具有研发经验、熟悉药品相关法律法规的人才。",2019," "," "," "]
[" "," ",49,"生物医药及先进医疗器械","生物医药医疗","长春","九台区","长春海恩得生物科技有限公司"," "," "," ","本公司现自主检测能力为：微生物检测，理化检测，理化检测方法部分为企业标准，没有国家标准。先于科研部分提出需求，设备不完善，技术不成熟，需要国家技术支持以及资金支持。",2019," "," "," "]
[" "," ",50,"人工智能机智能机器人","人工智能","长春","朝阳区","华芯智能驾驶技术有限公司"," "," "," ","双目汽车高级辅助驾驶系统（双目ADAS）   FPGA高级工程师，高级算法工程师，AI智能处理算法工程师。",2019," "," "," "]
[" "," ",51,"人工智能机智能机器人","人工智能","长春","朝阳区","长春众向机器人科技有限公司"," "," "," ","针对商用场景的机器人软、硬件开发研究  机械、计算机类相关老师、学生，具有研发能力。",2019," "," "," "]
[" "," ",52,"其他","纺织","辽源","辽源","吉林省东北袜业园热力有限公司"," "," "," ","纺织工业园区能源综合利用；火力发电厂节能减排；能源供应系统合理优化布局，包含电能、蒸汽输送优化配置；工业生产废气余热回收开发；污水处理新工艺研讨，污水处理污泥综合利用；印染及织造工序建设自动化无人工厂；热电厂节能减排；能源梯级利用。  电力专业、热能专业、给排水专业、自动化专业等技术团队或相关高级技术人员。",2019," "," "," "]
[" "," ",53,"其他","制造业","辽源","辽源","吉林迎新玻璃有限公司"," "," "," ","玻璃质量分析系统研究开发  1、本科以上计算机软件编程专业；  2、本科以上非金属材料专业或化工专业；  3、从事玻璃生产技术三年以上人员",2019," "," "," "]
[" "," ",54,"其他","其他","四平","四平","梨树县黑土地人才开发服务中心"," "," "," ","旅游管理与开发人才培训项目   乡村旅游管理与项目开发类人才",2019," "," "," "]
[" "," ",55,"其他","其他","长春","九台区","长春锴达电子科技有限公司"," ","   新能源产品研发，电锅炉设计、研发、制造、销售、安装及维修，节能环保设备、水处理产品代理销售，环保治理工程施工，锅炉改造技术咨询（依法须经批准的项目，经相关部门批准后方可开展经营活动）。已注销。"," ","1、专业人才匮乏（电气自动化人才当地几乎找不到）  2、研究项目申报科技成果难，设备检测难",2019," "," "," "]
[" "," ",56,"其他","建筑建材","长春","九台区","长春玛莎建材有限公司九台分公司"," "," "," ","1、干硬性混凝土和塑性混凝土的生产配比人员。  2、电气工程类技术人员。  3、自动化控制及生产巡视人员。  4、机械维修保养技术人员。  机械制图及产品创新类画图人员。前企业没有需要解决的技术难题，主要困难是建材生产原料,缺少专业技术人员",2019," "," "," "]
[" "," ",57,"农产品加工及绿色食品","农产品加工","长春","榆树市","吉林省陆路雪食品有限公司"," "," "," ","糯玉米深加工技术  1.农副食品深加工生产技术型人才，人才层次为中级人才，需求数量6人；  2.农副食品深加工营销型人才，人才层次为中级人才，需求数量15人。",2019," "," "," "]
[" "," ",58,"农产品加工及绿色食品","农产品加工","长春","榆树市","吉林农投榆树粮食仓储物流有限公司"," "," "," ","淀粉、变性淀粉生产、制造、研发及污水处理新技术  淀粉及变形淀粉生产、研发人员，污水处理新工艺研发人员，中高级职称以上，数量5人。",2019," "," "," "]
[" "," ",59,"农产品加工及绿色食品","农产品加工","吉林","舒兰","舒兰市金星精制米有限公司"," "," "," ","稻谷加工工艺改良与提升  1.粮食加工人员2名。精通稻谷加工技术，能够根据原料的变化，如水量、含杂量等对设备参数做出合理调整，保证稻谷加工产量及加工工艺。  2.粮食加工领域深加工产业专门科技人才3名。专门的科技人才，用于研究粮食加工的深度与精度，提升粮食加工的创新体系。",2019," "," "," "]
[" "," ",60,"农产品加工及绿色食品","农产品加工","四平","四平","吉林红嘴种猪繁育有限公司"," "," "," ","干扰素诱导技术在猪病防治中的应用  畜牧兽医专业双师型高级人才，3—5人。畜牧兽医专业专科以上技术员若干人。",2019," "," "," "]
[" "," ",61,"农产品加工及绿色食品","农产品加工","白山","白山","白山现代农业有限公司"," "," "," ","人参皂苷Rg3提取中试生产技术红参有效成分提取中试技术   人参开发专业技术人才、高级营销人才",2019," "," "," "]
[" "," ",62,"农产品加工及绿色食品","农产品加工","白山","白山","白山市吉品生物科技有限公司"," "," "," ","低温纳米材料的配方研究   生产工艺研发，管理人员，市场运营人员等，预计30人",2019," "," "," "]
[" "," ",63,"农产品加工及绿色食品","农产品加工","白城","通榆","通榆益发合大豆制品有限公司"," "," "," ","提高大豆分离蛋白得率、废水综合利用提取大豆功能因子",2019," "," "," "]
[" "," ",64,"农产品加工及绿色食品","农产品加工","白城","通榆","吉林维多利农牧业有限公司"," "," "," ","牛屠宰与加工产品技术",2019," "," "," "]
[" "," ",{"$f":"ROW()-2","v":65},"农产品加工及绿色食品","农产品加工","长春","九台区","九台广源牧业有限公司"," "," "," ","网络销售，产品营销，奶牛繁殖，疾病防控。专利运用需要技术支持。",2019," "," "," "]
[" "," ",66,"农产品加工及绿色食品","农产品加工","长春","九台区","吉林省牧硕养殖有限公司"," "," "," ","1.养殖产生的粪尿可制作成机液肥，该项目在实验研发阶段，希望能在技术和信息上给予支持。  2.部分奶牛疾病的预防与治疗手段/方法需进一步提升，如乳房炎、子宫炎、蹄病等病理，需要监测、检测硬件与培训上的支持。  3.在养殖过程中，奶牛发情揭发率依旧比国外低，如何能提高发情揭发率，需要信息与技术上的支持。  4.检化验过程中微生物致病菌培养、药敏试验，技术薄弱、实验室标准较低，需要检测硬件、信息、技术上的支持。  5.如何提高饲料转化率，需要相关信息、技术上的支持。  6.奶厅牛只挤奶识别准确率低，无法正确分析挤奶数据（涵盖效率、奶产量、电导率、乳成分等），更谈不上繁殖数据（涵盖输精、流产、妊娠等）、兽医保健（涵盖揭发病牛、跟踪治疗等）、饲养管理（涵盖活动量、体重、舒适度、营养监控等）等生产相关数据的有效统计分析。",2019," "," "," "]
[" "," ",67,"农产品加工及绿色食品","农产品加工","长春","九台区","吉林省田野泉酿造有限公司"," "," "," ","新型豆酱产品是近几年发展起来的,它是在传统制酱的基础上,添加了具有特殊风味或保健功能的产品,已成为人们日常生活中不可缺少的一部分,但传统豆酱因其制作工艺原始，风味差异较大，无法实现产品标准化、工业化生产。针对传统大豆酱稳定性差、风味口感差异大、保质期短等无法实现工业化生产的瓶颈问题，需要进行民族特色食品加工过程中风味物质和质构特征形成及调控机制研究，挖掘传统工艺，开展民族区域特色原料品质筛选、工业化产品品质保真、风味物质的动态稳定监控研究，如何实现我国民族特色食品由传统手工作坊式制作向现代化大工业生产的升级？如何提高产品附加值，如何进行新型大豆酱制品产业化，如何给古老的豆酱加工行业注入了新的活力？怎样才能开发出了高品质新型大豆酱产品，提高大豆酱加工企业科技水平，加速企业向高科技迈进，实现产品升级产业化。",2019," "," "," "]
[" "," ",68,"农产品加工及绿色食品","农产品加工","长春","九台区","长春市隆达饲料有限公司"," "," "," ","1.青贮窖的建造技术  2.青贮饲料的加工与贮藏技术",2019," "," "," "]
[" "," ",69,"其他","建筑建材","长春","朝阳区","长春宏裕网架结构有限责任公司"," "," "," ","大跨屋盖建筑结构体系防灾自动化监控可行性研究   结构专业高级工程师10人，自动化电器专业高级技术人员5人，信息管理人员5人。",2019," "," "," "]
[" "," ",70,"其他","建筑建材","长春","朝阳区","吉林恒基建设投资集团"," "," "," ","三维激光扫描作业技术规程城镇道路再生沥青混凝土路面工程技术标准   测绘工程（教授）、工程测量（教授、副教授）、遥感技术（副教授）、摄影测量（讲师）道路工程（教授、副教授、讲师）",2019," "," "," "]
[" "," ",71,"其他","建筑建材","长春","南关区","长春市房多美绿色房屋股份有限公司"," "," "," ","装配一体化建筑外围护墙板的产业化研究  建筑1人，结构2人，材料2人",2019," "," "," "]
[" "," ",72,"其他","建筑建材","长春","南关区","吉林省誉衡工业电气有限公司"," "," "," ","集中供热系统动态精准调控关键技术   计算机软件研发：2～3人，本科及以上；电气自动化控制：4～5人，本科及以上；",2019," "," "," "]
[" "," ",73,"其他","建筑建材","四平","四平","四平市长城建筑材料有限公司"," "," "," ","攻关如何在节约成本的前提下优化建筑废弃物再生产砌块的性能   我公司需求建筑施工和工程材料领域技术指导及研发人才。",2019," "," "," "]
[" "," ",74,"其他","建筑建材","白城","白城","洮南市金石新型建材有限公司"," "," "," ","秸秆生态墙板提升技术  急需新型建材领域吉林省高级专家、长白山学者特聘教授等我省高层次专家以及建材专业博士、硕士和本科毕业生10名。",2019," "," "," "]
[" "," ",75,"其他","建筑建材","白城","白城","吉林徽商特种电缆有限公司"," "," "," ","新能源、环保耐火、电线电缆设备改造与技术升级",2019," "," "," "]
[" "," ",76,"其他","建筑建材","长春","九台区","建华建材（吉林）有限公司"," "," "," ","1.生产产生余浆（主要成分为胶凝材料、外加剂、砂与泥粉）外卖，未能循环利用转化成产品；  2.生产制造过程中产生废料未能再利用转化成产品。",2019," "," "," "]
[" "," ",77,"光电子及智能传感器","电子信息","长春","宽城区","吉林省众森永益科技有限公司"," "," "," ","1.单片机控制系统开发  2.机械手结构及驱动系统设计   单片机程序开发、机械手结构工程师;高技术人才；需求人数6人",2019," "," "," "]
[" "," ",78,"光电子及智能传感器","电子信息","长春","南关区","长春金阳高科技有限责任公司"," "," "," ","校园学生考勤及行为轨迹数据采集、身份识别多功能电子班牌关键技术",2019," "," "," "]
[" "," ",79,"光电子及智能传感器","电子信息","长春","二道区","闻鼓通信科技股份有限公司"," "," "," ","信息安全类高精尖技术  嵌入式底层研发人员、信息安全相关研发人员、大数据相关研发人员、  Web相关研发人员",2019," "," "," "]
[" "," ",80,"光电子及智能传感器","电子信息","长春","朝阳区","长春市朝阳区达内职业培训学校"," "," "," ","联合达内共建实验室   需求信息技术及机械类各专业，面向本科及以上相关专业人才，每年需求量为80-120人。",2019," "," "," "]
[" "," ",81,"光电子及智能传感器","电子信息","长春","朝阳区","长春市南北科技有限公司"," "," "," ","关于企业分销商城APP的研发  院校：长春理工大学长春大学院系：计算机系专业：前端开发工程师php后台开发工程师前端页面设计师人数：10人",2019," "," "," "]
[" "," ",82,"光电子及智能传感器","电子信息","长春","朝阳区","长春烽火技术有限公司"," "," "," ","线缆用自动收线技术  机电一体化专业，本科以上，1人",2019," "," "," "]
[" "," ",83,"光电子及智能传感器","电子信息","长春","朝阳区","吉林求是光谱数据科技有限公司"," "," "," ","低功耗型光机电一体机技术开发  专业领域：光学、电子学、计算机、机械  人才层次：博士、硕士、本科数量：30人",2019," "," "," "]
[" "," ",84,"光电子及智能传感器","电子信息","长春","二道区","长春易励光电仪器有限公司"," "," "," ","变焦镜头镜筒精密加工技术；红外加热靶标技术研究；   1.所需专业领域  本企业需求光电技术领域、精密机械制造领域、精密机械设计领域、仪器仪表领域的技术人才。  2.人才层次  技术人才的需求上，后备人才需求本科及以上学历为主，其他人才以具有一定经验的大专及以上人才为主。",2019," "," "," "]
[" "," ",85,"光电子及智能传感器","电子信息","长春","朝阳区","吉林省恒华光电有限公司"," "," "," ","光学透镜产品设计  院校：长春理工大学光电信息学院专业：光电专业人数：2人",2019," "," "," "]
[" "," ",86,"精密仪器及先进装备","装备制造","白城","白城","白城福佳科技有限公司"," "," "," ","多材料组分交界面X射线在线扫描检测系统研发。   光学：博士以上，2人、精密仪器：硕士以上，2人、电子与信息工程：硕士以上，2人。",2020," "," "," "]
[" "," ",87,"精密仪器及先进装备","装备制造","四平","四平","吉林世宝机械制造有限公司"," "," "," ","转向系统产品开发，过程软件开发   1.转向系统产品开发工程师2名；  2.转向系统过程开发工程师2名；  3.自动线软件设计开发工程师2名。",2020," "," "," "]
[" "," ",88,"精密仪器及先进装备","装备制造","白山","白山","吉林木果科技有限公司"," "," "," ","1.软件工程师：独立开发软件，会编程，数据库技术；  2.硬件工程师：嵌入式硬件开发设计；  3.机械设计师：会机械设备设计。  文员3名、财务2名、平面设计师、高级操作工10、软件工程师、硬件工程师、股份制店长、机械设计师。",2020," "," "," "]
[" "," ",89,"精密仪器及先进装备","装备制造","吉林","吉林","吉林金洪汽车部件股份有限公司"," "," "," ","1.旋转攻丝铆接（FDS）；  2.自动铆接(SPR)；  3.无铆铆接（TOX）；  4.铝产品焊接；  5.自动化调整:1250T现有部分产品没有实现自动化；  6.防错的应用：现焊接产品只能防止漏焊，错焊无法防错；  7.弧焊气孔：现有部分产品弧焊气孔无法解决；  8.激光焊接检验：现激光焊接无法实现在线监测；  9.数据收集：焊接参数、质量监控数据现无法实现在线收集；  10.用冷冲压工艺、以钢板为毛坯制做螺母，差在冲压模具内实现攻丝；  11.凸焊螺母焊接飞溅检测技术。   铝焊接人才。",2020," "," "," "]
[" "," ",90,"碳纤维及复合材料","新材料","白山","白山","吉林蓝锐电子科技有限公司"," "," "," ","液冷LED路灯材料替换及灌注  需要工程管理人才一人，本科学历。",2020," "," "," "]
[" "," ",91,"精细化工及天然气化工","新材料","白山","白山","白山喜丰塑业有限公司"," "," "," ","减少流滴剂各组分中混入的杂质；对流滴剂采用丙烯酸接枝技术予以改性处理。   化工15人机械、电气6人均为大专以上学历。",2020," "," "," "]
[" "," ",92,"生物基新材料","新材料","白山","临江","临江市瑞丰植物纤维制品有限公司"," "," "," ","可降解农用地膜生产工艺。  可降解地膜生产领域、本科以上学历、人数为2人。",2020," "," "," "]
[" "," ",93,"碳纤维及复合材料","新材料","延边州","敦化","吉林德蕴电气集团股份有限公司"," "," "," ","大型变电站整体预制舱防腐、保温、抗寒、结构强度，机械制造设计、机械工业美学设计、电气工程及其自动化。  具备高级职称的结构工程师及电气工程师两方面人才各10-20人。",2020," "," "," "]
[" "," ",94,"碳纤维及复合材料","新材料","长春","绿园区","吉林省泽赛新材料有限公司"," "," "," ","1.高分子弹性体动静态力学实验技术；  2.高分子弹性体物理性能应用技术；  3.噪声与振动控制技术；  4.火灾防火类产品、防火涂料、防火封堵产品的设计研发、市场应用、性能检测；  5..电力、石化、基础建筑等行业的消防验收流程；  6.液体产品的保质期（使用寿命）的快速检验测试方法；  7.政府资金及政策支持。",2020," "," "," "]
[" "," ",95,"精细化工及天然气化工","新材料","长春","朝阳区","长春三友智造科技发展有限公司"," "," "," ","1.研发具有自主知识产权的新型开环易位催化乙烯，考察不同过渡金属配合物对环境稳定性和催化活性的影响规律；  2.研究国产双环戊二烯原料纯度与催化活性、固化程度的关系，优化出具有优异机械强度、热稳定性和良好成型工艺性的聚双环戊二烯组合料生产工艺；  3.研究不同阻燃剂与聚双环戊二烯组合料的相容性规律，考察影响阻燃效果的因素，开发出具有良好阻燃性的烯材料；  4.研究聚双环戊二烯与纤维材料的复合工艺  5.研究聚双环戊二烯不同应用场景的性能改性  6.研究聚双环戊二烯产品的回收利用，可持续发展产业链  院士1人高分子材料/阻燃/可回收  博士5人高分子材料/催化剂/纤维复合  硕士10人机械设计/化学分析/模具设计",2020," "," "," "]
[" "," ",96,"碳纤维及复合材料","新材料","吉林","吉林","吉林唯圣能源科技开发有限公司"," "," "," ","1.矿渣中二氧化硅的提取  2.废渣的综合利用  材料化学、无机材料、化学工程相关专业5人，高等院校全日制本科或硕士以上学历，最好有1年以上相关研发工作经验。可独立完成工艺制定、实施监督工作。",2020," "," "," "]
[" "," ",97,"碳纤维及复合材料","新材料","吉林","吉林","吉林莱德化学科技有限公司"," "," "," ","1.锌及锌合金无铬钝化剂  2.水性无铬锌铝涂料  3.汽车专用化学品  4.水性钛酸酯偶联剂",2020," "," "," "]
[" "," ",98,"生物医药及先进医疗器械","生物医药医疗","长春","二道区","长春赛诺迈德医学技术有限责任公司"," "," "," ","1.机器人导航技术  2.免疫试剂技术   硕士学历以上，软件研发工程师2人、测量研发工程师1人、试剂研发工程师6人，机器人相关工程师4人，光学工程师1人。",2020," "," "," "]
[" "," ",99,"生物医药及先进医疗器械","生物医药医疗","辽源","辽源","吉林省博大制药股份有限公司"," "," "," ","1.阿哌沙班原料及制剂生产工艺  2.舒更葡糖钠原料及制剂的生产工艺   1.药品研发管理，研究生及以上。2人  2.药品研发制剂方向，本科生及以上，2人  3.药品研发原料方向，本科生及以上。2人（所需专业领域、人才层次及数量要求）",2020," "," "," "]
[" "," ",100,"生物医药及先进医疗器械","生物医药医疗","白山","白山","吉林长白山药业集团股份有限公司"," "," "," ","在中药材提取挥发油过程中，挥发油大量损失及提取率偏低，致使挥发油有效成分和保留存在着很多问题，影响了药物的疗效。确定科学合理的提取时间来确定挥发油提取工艺参数   化工药品分析10人",2020," "," "," "]
[" "," ",101,"生物医药及先进医疗器械","生物医药医疗","通化","梅河口","弘和制药有限公司"," "," "," ","1.心脑血管领域  2.以大容量注射剂为主  3.适用于大输液生产  4.化学药研发技术",2020," "," "," "]
[" "," ",102,"生物医药及先进医疗器械","生物医药医疗","通化","梅河口","吉林天成制药有限公司"," "," "," ","多组分生化药工艺提升  需要药学专业人才",2020," "," "," "]
[" "," ",103,"生物医药及先进医疗器械","生物医药医疗","通化","梅河口","通化谷红制药有限公司"," "," "," ","中药质量再评价研究   药学专业技术人才",2020," "," "," "]
[" "," ",104,"生物医药及先进医疗器械","生物医药医疗","长春","双阳区","吉林省吉诺生物工程有限责任公司"," "," "," ","  特医食品技术开发及产业化     食品、药学、生物、营养、医学等相关专业领域人才，熟悉体外诊断产品或生物技术产品开发经验。",2020," "," "," "]
[" "," ",105,"生物医药及先进医疗器械","生物医药医疗","长春","双阳区","长春卓谊生物股份有限公司"," "," "," ","  轮状病毒疫苗     专业领域：病毒疫苗研究相关专业；  人才层次：硕士研究生以上学历；  数量要求：20人-30人",2020," "," "," "]
[" "," ",106,"人工智能机智能机器人","人工智能","长春","宽城区","长春光华科技发展有限公司"," "," "," ","  人工智能领域  1.卷积神经网络深度学习算法  2.活体人脸算法模型  3.自主导航slam算法     数据工程师  1.数据架构师2人；2.数据开发5人；3.数据挖掘5人  软件研发  1.微服务Java架构师2人；2.微服务Java研发工程师5人；3.C++研发工程师5人；4.Python研发工程师5人；5.嵌入式软件开发5人；6.Bootstrap前端研发工程师5人；  硬件研发  1.C语言研发工程师5人；2.ARM研发工程师5人",2020," "," "," "]
[" "," ",107,"精密仪器及先进装备","装备制造","吉林","桦甸","吉林圆方机械集团有限公司"," "," "," ","  1.现有半轴、轴管材质40Cr、30Mn2，锻造后毛坯通过调质处理表面至心部10mm处组织要求达到索氏体1-4级；  2.磁粉探伤机能否实现自动探伤、自动分选不合格品、消除人为因素的影响，杜绝不合格品混入合格品中；  3.半轴毛重在22-35KG，上、下工件、搬运劳动强度大，争取实现上、下工件、搬运自动化、机械化，同时不能降低生产效率、降低劳动强度、实现少人化生产。",2021," "," "," "]
[" "," ",108,"精密仪器及先进装备","装备制造","辽源","辽源","辽源市万通汽车部件有限公司"," "," "," ","  1.汽车铸造零部件QT600-5材质的研究；  2.汽车车身智能网联的产品研究。",2021," "," "," "]
[" "," ",109,"精密仪器及先进装备","装备制造","长春","绿园区","一汽集团研发总院试制所"," "," "," ","  DHT差速器总成由差速器壳体和从动齿轮组成，焊接时为球墨铸铁和钢焊接，焊接极易产生气孔、裂纹等缺陷，该总成为高扭矩零件，对焊缝质量及焊接小变形要求很高，需要通过技术研究，确定合适的激光焊接工艺方法。",2021," "," "," "]
[" "," ",110,"精密仪器及先进装备","新能源","吉林","蛟河","蛟河凯迪绿色能源开发有限公司"," "," "," ","  蛟河凯迪绿色能源开发有限公司利用蛟河当地的农业秸秆和林业废弃物等“绿色能源”作燃料发电，发电剩余生物质灰渣想加工成砖。",2021," "," "," "]
[" "," ",111,"精细化工及天然气化工","新材料","长春","绿园区","长春市汇融密封材料有限公司"," "," "," ","  随着技术发展及制造工业自动化程度飞跃提高，我们公司发展到瓶颈，二大问难题亟待解决，一是产品技术更新换代研发能力，寻求高水平材料研究科研单位合作共同开发换代产品,二是新型环保水性胶粘剂项目合作开发问题。  ",2021," "," "," "]
[" "," ",112,"碳纤维及复合材料","新材料","长春","绿园区","长春一汽四环汽车管路有限公司"," "," "," ","  随着科技的进步和汽车行业的发展，不同客户对管体的要求也不断提高。  1、对管体的阻燃性；  2、提高尼龙管的弹性；  3、在性能不变的同时如何降低成本；  4、减低管体的析出。",2021," "," "," "]
[" "," ",113,"农产品加工及绿色食品","食品加工","白山","抚松","吉林长白明珠森林食品有限公司"," "," "," ","  蓝莓果酱的制作方法、保鲜山野菜的制作方法、酱制食用菌的制作方方法",2021," "," "," "]
[" "," ",114,"农产品加工及绿色食品","食品加工","吉林","桦甸","吉林出彩农业产品开发有限公司"," "," "," ","  解决中低温豆粕深加工蛋白水溶性差的问题，紫苏油、葡萄籽油精练技术",2021," "," "," "]
[" "," ",115,"农产品加工及绿色食品","食品加工","吉林","桦甸","桦甸市金牛牧业有限公司"," "," "," ","  1、牛肉酱，目前自己在做，但不知道如何延长保质期；瓶包装盒塑料包装目前都有；自己有个配方，目前还想引进配方。  2、牛肉干产品。",2021," "," "," "]
[" "," ",116,"农产品加工及绿色食品","食品加工","吉林","桦甸","吉林省田谷有机食品有限公司"," "," "," ","  1、酸菜衍生品加工，如即食酸菜等产品；  2、酸菜销售一段时间易发黑、发生褐变；  3、加工过程中损耗大，有很多白菜帮等损失，如何解决？",2021," "," "," "]
[" "," ",117,"精细化工及天然气化工","石油化工","延边州","延吉","吉林长白山包装材料有限公司"," "," "," ","  我厂在生产烟用接装纸时在产品的表面需要印刷一层带甜味的光油（油墨），光油的主要成分：改进松香+酒精+甜菊糖苷。按照配方比例调整好的光油经印刷机（网纹版转移方式，需要循环使用）印刷到产品表面。现况为：光油使用过程中会逐渐增稠，在使用到3-4小时后印刷的产品表面触摸会有颗粒感，此时生产的产品相比正常产品味觉甜度更甜，但经设备检测每公斤产品中甜味剂含量低于未析出的正常产品（产品需味觉、含量两项指标都符合标准）。",2021," "," "," "]
[" "," ",118,"精细化工及天然气化工","石油化工","四平","四平","吉林省新天龙实业股份有限公司"," "," "," ","  企业目前正在进行以玉米秸秆为原料生产酒精的项目研发，项目中的原料收集、预处理、糖化等工艺过程以及发酵菌、酶制剂的成本是整个纤维素乙醇生产的制约，解决好每个单元才能实现纤维素乙醇的真正产业化。",2021," "," "," "]
[" "," ",119,"生物医药及先进医疗器械","生物医药医疗","长春","宽城区","吉林大北农农牧科技有限责任公司"," "," "," ","  中药渣通过生物发酵或膨化完全可以改善原料风味、增加纤维利用率、增加活菌代谢产物形成具有一定功能性的饲料原料使用。而且生产的发酵中药渣或膨化中药渣各项指标均达到或超过目前的常规纤维饲料原料，同时我省有丰富的中药渣资源，因此针对该现状选育微生物功能菌株，组合成有益复合微生物菌剂，研究其最佳培养条件和特殊的发酵工艺，以中草药药渣为原料，配合其它饲料原料进行发酵的中药渣资源饲料化生物利用关键技术及产业化示范应用项目发展潜力巨大。",2021," "," "," "]
[" "," ",120,"生物医药及先进医疗器械","生物医药医疗","吉林","磐石","磐石巨康药业有限公司"," "," "," ","  高压蒸汽灭菌后有沉淀产生。  改变法定工艺或不改变法定工艺。如改变法定灭菌工艺需做药学等方面的研究，费时费力但结果未知。",2021," "," "," "]
[" "," ",121,"生物医药及先进医疗器械","生物医药医疗","长春","朝阳区","迪瑞医疗科技股份有限公司"," "," "," ","  磁颗粒作为IVD固相捕获用原材料，主要用于捕获抗体抗原反应物，在磁场作用下，实现被测物与未反应物的分离。IVD磁颗粒原材料性能直接影响IVD产品的核心性能指标。  当前IVD磁颗粒主要依赖进口（如赛默飞和捷时雅等厂家），国产磁珠在粒径均一性、表面官能团参数等方面不能满足IVD产品试剂灵敏及线性需求，因此开发设计功能性磁珠，最后包被链酶亲和素，制备链酶亲和素磁珠产品势在必行。",2021," "," "," "]
[" "," ",122,"人工智能机智能机器人","人工智能","长春","南关区","易启科技（吉林省）有限公司"," "," "," ","  图像或造型数据采集的成像技术：需要一种能够覆盖较大面积（例如1㎡）具有一定造型的、达到微米级精度，且在较短时间内（例如8s）完成图像或造型数据采集的成像技术。     计算机视觉专业人才，博士后/博士/硕士光学专业人才，博士后/博士/硕士机械及自动化专业人才，博士/硕士计算机类专业人才，硕士/本科",2021," "," "," "]
[" "," ",123,"光电子及智能传感器","电子信息","长春","朝阳区","长春希达电子技术有限公司"," "," "," ","  1.三基色MiniLED背光技术尚处于技术积累阶段，技术成熟度较低，在三基色MiniLED背光模组集成封装、三基色MiniLED背光驱动控制、高精度光电参数采集及均一性调控等方面还面临许多问题。  2.需求非接触EL方式实现MicroLED器件高效缺陷检测技术项目的支持。",2021," "," "," "]
[" "," ",124,"精密仪器及先进装备","装备制造","长春","绿园区","中车长春轨道客车股份有限公司"," "," "," ","  1.列车网络安全项目；  2.未来高铁被动安全关键技术研究项目；  3.轨道交通车辆车厢声场优化研究项目；  4.高速动车组时空精准稳定定位技术研究；  5.动车组高压绝缘材料技术研究项目；  6.动车组转向架装配数字化产线建设项目；  7.城市轨道交通应用氢能源技术研究项目；  8.超导电动磁浮车轨桥隧耦合动力学特性及参数匹配设计研究项目；  9.产用一体化绿色电力工业应用项目。",2022," "," "," "]
[" "," ",125,"精密仪器及先进装备","装备制造","白城","白城","白城天奇装备机械有限公司"," "," "," ","  机械电气专业应届毕业生2人、电气专业职业技术工人1人。",2022," "," "," "]
[" "," ",126,"精密仪器及先进装备","装备制造","延边州","敦化","亚联机械股份有限公司"," "," "," ","  “双一流”机械电气专业应届毕业生10人、机械专业职业技术工人5人、机械电气高级技术人才7人。",2022," "," "," "]
[" "," ",127,"精密仪器及先进装备","装备制造","延边州","延吉","延边国泰新能源汽车有限公司"," "," "," ","  “双一流”车辆工程、机械设计、控制工程等相关专业应届毕业生2人、普通应届生3人。",2022," "," "," "]
[" "," ",128,"精密仪器及先进装备","装备制造","辽源","辽源","格致汽车科技股份有限公司"," "," "," ","  欧标模具铸钢件铸造、加工、表面淬火处理等工序的生产技术标准。",2022," "," "," "]
[" "," ",{"$f":"ROW()-2","v":129},"精密仪器及先进装备","装备制造","白城","白城","中材科技（白城）风电叶片有限公司"," "," "," ","  大叶型风力发电叶片技术开发。    复合材料专业硕士毕业生2人、本科毕业生10人。",2022," "," "," "]
[" "," ",130,"精密仪器及先进装备","新能源","白城","大安","吉林重通成飞新材料股份公司"," "," "," ","  CGI90+碳纤维超长尺寸超大容量风电叶片关键技术突破与应用及资金投入",2022," "," "," "]
[" "," ",131,"碳纤维及复合材料","新材料","辽源","辽源","吉林省华纺静电材料科技有限公司"," "," "," ","  低气味PP/麻纤维复合材料制备关键技术研究。    高分子、材料学专业高级技术人才1-2人。",2022," "," "," "]
[" "," ",132,"碳纤维及复合材料","新材料","辽源","辽源","吉林省正轩车架有限公司"," "," "," ","  机械专业普通高校本科毕业生2人、中专技术工人19人。",2022," "," "," "]
[" "," ",133,"碳纤维及复合材料","新材料","通化","通化县","通化宏信研磨材有限责任公司"," "," "," ","  碳化硅陶瓷制品的生产工艺。",2022," "," "," "]
[" "," ",134,"农产品加工及绿色食品","现代农业","长春","南关区","吉林省农业综合信息服务股份有限公司"," "," "," ","  “双一流”计算机专业本科毕业生2人、普通高校毕业生2人、大专职业技术工人2人、高级程序技术人才2人。",2022," "," "," "]
[" "," ",135,"农产品加工及绿色食品","食品加工","通化","通化县","通化禾韵现代农业股份有限公司"," "," "," ","寒地蓝莓规模化种植项目  果蔬种植及园艺类普通高校本科毕业生5人。",2022," "," "," "]
[" "," ",136,"农产品加工及绿色食品","食品加工","通化","通化县","通化通天酒业有限公司"," "," "," ","东北浆果饮料酒的研发生产    药学专业博士应届毕业生1人、硕士毕业生1人、“双一流”药学专业本科毕业生3人、普通高校毕业生5人、大专职业技术工人5人、中专职业技术工人5人、负责生产/质量/销售高级管理人才3人、负责研发高级技术人才3人、负责生产技术工程师2人。",2022," "," "," "]
[" "," ",137,"农产品加工及绿色食品","食品加工","通化","通化县","通化青山实业集团有限公司"," "," "," ","  需要成套生产解决方案。",2022," "," "," "]
[" "," ",138,"生物医药及先进医疗器械","生物医药医疗","延边州","延吉","吉林敖东药业集团延吉股份有限公司"," "," "," ","  开发大容量注射剂新产品    制药专业普通应届生5人。",2022," "," "," "]
[" "," ",139,"生物医药及先进医疗器械","生物医药医疗","延边州","龙井","吉林延边朝药药业有限公司"," "," "," ","  “双一流”药学专业应届毕业生2人、药学专业职业技术工人4人、药学专业高级技术人才2人。",2022," "," "," "]
[" "," ",140,"生物医药及先进医疗器械","生物医药医疗","通化","通化县","通化华夏药业有限责任公司"," "," "," ","  药学博士2人",2022," "," "," "]
[" "," ",141,"生物医药及先进医疗器械","生物医药医疗","通化","通化县","通化东宝药业股份有限公司"," "," "," ","  药学专业博士应届毕业生2人、硕士毕业生20人、“双一流”药学专业本科毕业生10人、普通高校毕业生100人、大专职业技术工人30人、中专职业技术工人20人。",2022," "," "," "]
[" "," ",142,"生物医药及先进医疗器械","生物医药医疗","通化","通化县","通化白山药业股份有限公司"," "," "," ","需要药学专业博士2人",2022," "," "," "]
[" "," ",143,"生物医药及先进医疗器械","生物医药医疗","通化","通化","通化康元生物科技有限公司"," "," "," ","  药学专业博士应届毕业生1人、硕士毕业生1人、“双一流”药学专业本科毕业生3人、普通高校毕业生5人、大专职业技术工人5人、中专职业技术工人5人、负责生产/质量/销售高级管理人才3人、负责研发高级技术人才3人、负责生产技术工程师2人。",2022," "," "," "]
[" "," ",144,"生物医药及先进医疗器械","生物医药医疗","四平","四平","比智高药业有限公司"," "," "," ","  需要成套生产解决方案",2022," "," "," "]
[" "," ",145,"生物医药及先进医疗器械","生物医药医疗","通化","通化县","吉林省通化振国药业有限公司"," "," "," ","  口服液二次研发项目",2022," "," "," "]
[" "," ",146,"生物医药及先进医疗器械","生物医药医疗","通化","通化","东方红西洋参药业（通化）股份有限公司"," "," "," ","  食品提取酶解技术及中药配方颗粒研究    食品工程专业普通高校毕业生2-3人。",2022," "," "," "]
[" "," ",147,"生物医药及先进医疗器械","生物医药医疗","通化","柳河县","吉林省中晟制药有限公司"," "," "," ","  复方氨酚烷胺胶囊泛丸工艺研究；    药学专业普通高校毕业生5人、大专职业技术工人5人、高级技术人才3人。",2022," "," "," "]
[" "," ",148,"其他","生态环保","通化","通化县","吉林省拓达环保设备工程有限公司"," "," "," ","  适用于高寒地区村镇污水处理工艺技术的研发    “双一流”环境工程/给排水/电气/自动化专业本科毕业生4人、普通高校毕业生8人、大专职业技术工人8人。",2022," "," "," "]
[" "," ",149,"精密仪器及先进装备","装备制造","白城","镇赉","成来电气科技有限公司"," "," "," ","  真空灌注高性能风电机组舱罩成型关键技术研发（预算50万元）  项目采用长玻纤织物与短玻纤多层交替结构优化风电机组舱罩刚度，引入纳米结构的颗粒状无机硅填料，提高材料的有效利用率和减轻结构重量、增加基体综合性能，设计新型真空灌注模具，考察乙烯基热塑性树脂及长链丙烯酸酯类对玻纤、无机填料与不饱和树脂的结构影响，剖析分子化学键链相互作用机理，调控固化产品的收缩率，攻克多级真空联动灌注关键核心技术，实现低成本高稳定性的环保成型工艺，获得高精度的风力发电机舱罩产品。",2023," "," "," "]
[" "," ",150,"精密仪器及先进装备","装备制造","长春","绿园区","一汽模具制造有限公司"," "," "," ","  新能源铝合金电池壳体焊接变形控制技术（100万元）  研究开发新能源铝合金电池壳体焊接工艺技术装备，重点攻克铝合金电池壳体焊接变形控制关键技术。研发电池壳体焊接专业试验台，通过研究焊接变形的仿真优化、焊前预处理方法、焊接夹具反变形、焊接电流、焊接速度、焊道焊接工艺顺序的优化控制、焊接去应力等综合变形控制技术，实现对电池壳体焊接变形的控制。",2023," "," "," "]
[" "," ",151,"精密仪器及先进装备","装备制造","长春","九台区","长春数控机床有限公司"," "," "," ","  航空发动机转子超重型惯性摩擦焊机主轴静压轴承（预算3000万元）  航空发动机转子超重型惯性摩擦焊机主轴静压轴承(轴向力1000T,转速400RPM,回转精度0.04mm)设计与制造。",2023," "," "," "]
[" "," ",152,"精密仪器及先进装备","装备制造","长春","朝阳区","吉林省先达条码信息技术有限公司"," ","吉林省先达条码信息技术有限公司是由长春理工大学、先达集团（兵器工业直属）与先达科技系统（深圳）有限公司共同出资组建的合资企业，地址位于长春理工大学科技园内，是吉林省内比较专业的集条码技术、IC卡技术、射频技术等自动识别技术为一体的高新技术企业。公司于2006年加入了中国自动识别技术协会，成为协会会员单位，于2006年获得了吉林省双软企业认证，于2006年成为“中国条码推进工程”参与单位。  "," ","  用于视觉检测的可借用测试的工业光源。",2023," "," "," "]
[" "," ",153,"精密仪器及先进装备","装备制造","长春","朝阳区","东北工业集团  吉林东光集团有限公司"," ","吉林东光集团有限公司（曾用名：吉林东光汽车零部件有限责任公司），成立于1956年，位于吉林省长春市，是一家以从事仪器仪表制造业为主的企业。是我国“一五”期间原苏联援建的156个重点项目之一。是全国四大光学研究生产基地之一，是以光学仪器制造为主的企业，坐落在吉林省长春市高新技术产业开发区内。现有职工300余人，其中科技人员119人，工程师以上58人，高级工程师20人。  光学研发中心具备国内较强的精密光学产品开发能力，拥有一批达到国际先进水平的数控加工中心、光学镀膜中心等先进的生产设施，形成了较为完备的超精密光学加工能力。业务涵盖武器装备科研生产、汽车零部件、光学仪器、铸件、锻件、机械加工制造、经营本企业自产产品及相关技术的出口业务、本企业生产、科研所需原辅材料、设备及技术的进口业务等。企业注册资本30000万人民币，实缴资本30000万人民币。"," ","  图像目标识别模块处理-预算5万可见光图像和红外图像进行目标识别和图像融合处理。具有线上实时数字图像畸变校正功能；具有可见光/红外图像融合功能；具有目标检测功能。  高光谱成像模块-预算20万利用分光组件将进入模块的目标反射光按照不同波长分别成像在不同探测器上，实现对目标光谱特征的探测。",2023," "," "," "]
[" "," ",154,"精密仪器及先进装备","装备制造","长春","宽城区","长春日辰光电技术有限公司"," "," "," ","  光学设计大变倍比高清连续镜头压缩光学总长技术。  目前市场对此类产品需求是：体积小、重量轻，因此光学设计在压缩总长上十分重要。",2023," "," "," "]
[" "," ",155,"精密仪器及先进装备","装备制造","长春","南关区","吉林羽麦航空有限公司"," "," "," ","  不同行业高光谱原始数据库、基于FPGA高光谱图像处理软硬件、高精度地磁测量传感器的国产化。  针对不同行业对原始数据进行解译、处理、模型训练。生成对特定行业数据处理的算法；需要FPGA软硬件开发人员；国产化地磁测量传感器与国外同类型设备测量精度一致。该系统的应用场景将包括但不限于海洋污染预警探测（海洋污染、叶绿素监测、温度监测）、生态保护（水体污染、排污口监测、岸线调查、覆被分类、生态绿化监测、水源地监测）、农林植被分析（发芽/抽穗率、株/行间距、节水灌溉智能识别、作物分类、健康状态分析、地形地势探测、病虫害、覆盖度、植被分类、生物入侵、成活率/长势监测）、应急救援（灾情监测、保险理赔、灾后重建、应急探测、广域搜索）、军警执勤（岛屿安防、边海防、周界管控、罂粟筛查、目标识别）。源于设备的高效、精准、先进，设备可以做到“只看所需，不止所见”，为需求用户提供全新的需求解决方案。",2023," "," "," "]
[" "," ",156,"精密仪器及先进装备","装备制造","长春","二道区","长春长光易格精密技术有限公司"," "," "," ","  熔模石膏型精密铸造铝合金结构件技术优化-预算100万  加快新一代合金铸造工艺的技术创新与升级,缩短与国际先进水平的差距,解决制约行业发展的难点痛点，力争攻克复杂结构、薄壁、提高力学性能等行业难题。",2023," "," "," "]
[" "," ",157,"精密仪器及先进装备","装备制造","长春","二道区","长春长光大器科技有限公司"," "," "," ","  数字化生产-预算20~30万  公司在加工定制服务和装备制造方面能对过程进行数字化描述，对装备的传感器进行数字化网络传输并记录。加工软件具备云服务器计算功能，与本地计算机形成功能分割。同时能把设备产生的实时数据上传至互联网，方便操作人员远程查看与记录。",2023," "," "," "]
[" "," ",158,"精密仪器及先进装备","装备制造","长春","二道区","长春长光奥闰光电科技有限公司"," "," "," ","  CMOS真空封装技术-预算面议  对我司现有的技术进行升级在保证探测器洁净度与平整度的条件下，将其进行真空封装工艺处理。真空度要求：10-5保证探测器正常运行密封度要求：至少5年之内不漏气。",2023," "," "," "]
[" "," ",159,"精密仪器及先进装备","装备制造","长春","宽城区","长春长光博翔无人机有限公司"," "," "," ","  高能量密度高功率高安全电池、-40℃特种高功率电池。",2023," "," "," "]
[" "," ",160,"精密仪器及先进装备","装备制造","长春","德惠市","吉林省汉华重型装备制造有限公司"," "," ","近年来，随着国家清洁能源战略的推进，风力发电铸件的需求量不断增加。东北地区风力资源丰富，市场潜力巨大。吉林汉华具有较为先进的技术、装备、市场、人才队伍、经营理念等基础条件，企业以技术创新为核心驱动力，为进一步发展，需要努力打造高端铸件市场竞争力。风力发电设备中的大型零件如轮毂、基座、主轴、行星架等都采用球墨铸铁生产。随功率的不同，重量在5000kg到50000kg之间，由于壁厚较厚(一般大于100毫米),重量较重，冷却速度慢，凝固时间长，且工况条件复杂，对铸件综合力学性能、内在质量等要求很高，生产技术难度较大。","  大型风力发电铸件关键技术研发  根据市场需求，结合企业自身优势，公司拟开展风力发电铸件关键技术研发，在材料力学性能提升(一般为QT400-18AL)、检验技术完善(MT、UT等)、造型工艺改进等方面有所突破，以助力企业综合竞争能力进步。项目完成后将实现年产铸件30000吨，产值3亿元，材质质量较一般标准提升一个牌号、制造成本下降10%以上。项目在大型厚壁球墨铸铁件造型、制芯、原材料质量控制、熔炼工艺优化、铸件无损检测、涂装、加工等关键技术的研究和改进，难度大、投入高，需要组建铸造工艺、熔炼材料、检验、加工等方面的专业团队，也希望能得到高校及业内专业人士的支持。",2023," "," "," "]
[" "," ",161,"精密仪器及先进装备","装备制造","长春","二道区","长春东北输送链条制造有限公司"," "," "," ","  智能化物流（预算5万元）  agv小车应用，受工作环境影响，无法应用。",2023," "," "," "]
[" "," ",162,"精密仪器及先进装备","装备制造","白城","大安","大安鸿源管业有限公司"," "," "," ","  采油井低成本实时含水率测量（2022）、引进数字化人才需求（2023）。",2023," "," "," "]
[" "," ",163,"精密仪器及先进装备","新能源","长春","九台区","吉林省中科电缆附件有限公司"," "," "," ","  ±500kV直流电力电缆附件产品设计（150万元）  1)成型工序良品率达到95%以上；  2)产品性能满足国标规定的预鉴定试验和型式试验要求。",2023," "," "," "]
[" "," ",164,"精密仪器及先进装备","新能源","长春","朝阳区","长春致远新能源装备股份有限公司"," "," "," ","  1、氢液化技术及配套工艺装备研发  2、液态氢加注核心装备技术研发",2023," "," "," "]
[" "," ",165,"精密仪器及先进装备","新能源","吉林","磐石","磐石市星环阀片有限公司"," "," "," ","  缺少技术工种人员",2023," "," "," "]
[" "," ",166,"碳纤维及复合材料","新材料","长春","朝阳区","长春市三化实业有限责任公司"," "," "," ","预算50万元  一.油性金属闪光挂车漆，包括双组份丙烯酸聚氨酯和醇酸漆。二.水性丙烯酸聚氨酯中涂漆和水性丙烯酸聚氨酯面漆。",2023," "," "," "]
[" "," ",167,"碳纤维及复合材料","新材料","长春","宽城区","长春市信安包装有限公司"," "," "," ","提高瓦楞纸箱生产工艺质量稳定性的关键技术  1、稳定高效的淀粉胶粘剂制备技术  (1)持续稳定的胶粘剂粘度和浓度；(2)胶粘剂无分层、凝沉和  水解现象。  2、优异的纸板贴合工艺  (1)提高涂胶均匀度；(2)提升纸板粘着强度。  3、工艺优化，降低能耗，提高生产车速。",2023," "," "," "]
[" "," ",168,"生物基新材料","新材料","长春","南关区","吉林中粮生化有限公司"," "," "," ","生物降解吸管改性料产业化研究与开发（预算60万元）  本项目是对降解高聚物改性和加工成型技术的集成，在不改变传统吸管的加工工艺以获得可完全生物降解吸管是本项目的核心技术。目前还没有单一的生物降解材料能够满足加工性、使用性能的要求，需要以多组分的方法制备专用树脂。优化专用树脂的组成，强化组分间的相容性；提高专用树脂的流变性能，满足制品加工成型工艺要求；调控专用树脂的结晶性，满足制品运输和使用时对耐温性要求；合理降低配方成本，以满足更好的市场应用与推广。  预期技术指标：  (1)拉伸强度≥40Mpa  (2)断裂伸长率≥20%  (3)总迁移量：4%乙酸(70℃,2h)≤10mg/dm²10%乙醇(70℃,2h)≤10mg/dm²",2023," "," "," "]
[" "," ",169,"碳纤维及复合材料","新材料","长春","南关区","吉林省新方圆检测认证股份有限公司"," "," "," ","新型墙体材料、节能保温材料研发与应用（预算100万元）  新型节能材料的研发与应用，保证节能保温效果(即导热系数满足要求)的前提下，研制轻型A级防火材料。  新型墙体材料，拟采用轻质材料或发泡材料作为主材，一次性浇筑，无需抹面，强度等级满足MU5.0及以上要求，有一定的隔音效果。",2023," "," "," "]
[" "," ",170,"碳纤维及复合材料","新材料","长春","绿园区","吉林省峰海工贸有限公司"," "," "," ","无机灌注型复合防火玻璃生产工艺提升  复合型灌封胶防火玻璃工艺问题：1.量产化问题；2.生产过程中气泡控制问题；3.灌封胶粘度问题(粘度大灌注很慢，影响生产效率)",2023," "," "," "]
[" "," ",171,"碳纤维及复合材料","新材料","长春","南关区","格拉默车辆内饰（长春）有限公司"," "," "," ","1.法规类国家更新信息通知  2.环保低碳材料信息",2023," "," "," "]
[" "," ",172,"精细化工及天然气化工","新材料","吉林","吉林","吉林恒昌科技股份有限公司"," "," "," ","关于车用PVC膜类胶水配方的研究  膜类产品的国产化替代方案，适时建立不干胶涂布线。  项目达成，降低我司原材料成本，增加我司竞争力；如果研发成功，自产不仅能满足公司自身需要，还可以推动对外销售原材料带来额外收益。",2023," "," "," "]
[" "," ",173,"碳纤维及复合材料","新材料","长春","朝阳区","鞍钢钢材加工配送（长春）有限公司"," "," "," ","国产低成本2GPa薄铝硅镀层热成形钢一体式双门环激光焊接关键技术开发与应用  \n(1)优化国产低成本2GPa薄铝硅镀层热成形钢不等厚板对接激光填丝  焊焊丝； \n(2)开发2GPa薄铝硅镀层热成形钢一体式双门环新结构及新加工方法；  \n(3)优化2GPa薄铝硅镀层热成形钢一体式双门环激光拼焊工艺窗口；  \n(4)不等厚热成形钢一体式双门环热成形试验验证。",2023," "," "," "]
[" "," ",174,"碳纤维及复合材料","新材料","长春","双阳区","长春铸诚实业股份有限公司"," "," "," ","多功能组合模块墙体技术研发（预算150万元）  竖龙骨的设计，嵌入式墙板密拼和带夹条的墙板与竖龙骨安装结合，横龙骨的设计与竖龙骨和墙板交接，天地轨的设计与墙体的安装，墙体的天地固定与地面高矮的调节，非金属板与墙体的安装结合同时与金属墙板结合，墙体与墙体连接形式结合窗(包括L型，丁字型，十字型等结合)门墙和窗墙结合，同时保证墙体各部件安装精度、隔音、保温、和安装强度达到国家标准。",2023," "," "," "]
[" "," ",175,"精细化工及天然气化工","新材料","长春","二道区","长春东狮科技（集团）有限责任公司"," "," "," ","新型窑炉煤气脱硫催化剂的研究  粉煤气化工艺50%以上的灰由煤气带出，致使煤气中的含尘量过高，一般废热锅炉出口处煤气中含尘量50g/m3左右。经洗涤、冷却、除尘捕滴，入脱硫煤气中含尘量仍然有80mg/m3左右。洗涤冷却过程中，洗涤冷却水质不能保证，进脱硫塔煤气含灰量过大；溶液中灰硫粘合颗粒过大，硫泡沫浮选不好；长期运行，填料层积灰、积硫，塔阻上升，脱硫效率下降；进塔溶液采用喷头的，易造成部分喷嘴堵塞，溶液偏流，脱硫效率下降。",2023," "," "," "]
[" "," ",176,"精细化工及天然气化工","新材料","长春","九台区","长春峰泰科技有限公司"," "," "," ","化工产品研发技术咨询服务。\n中小型企业融资服务。",2023," "," "," "]
[" "," ",177,"农产品加工及绿色食品","现代农业","长春","农安县","长春邦基宏运饲料有限公司"," "," "," ","解决非洲猪瘟，或者强力减缓非洲猪瘟的传播速度",2023," "," "," "]
[" "," ",178,"农产品加工及绿色食品","现代农业","白城","洮南","洮南圣一金地生物农业有限公司"," "," "," ","预算3万元  一年两茬种植技术及机械化、智能化生产模式。",2023," "," "," "]
[" "," ",179,"精密仪器及先进装备","先进制造","长春","朝阳区","长春禹衡光学有限公司"," "," "," ","超高精度光栅尺预算1000万  通过解决高精度光栅刻划、光电读数系统的设计、低噪声信号处理及反馈电路等技术问题，研制超高精度光栅尺。   \n技术指标：1、准确度：±0.5μm/m；2、栅距0.512μm；3、输出信号：～1Vpp；4、工作温度：-10℃至70℃；",2023," "," "," "]
[" "," ",180,"精密仪器及先进装备","先进制造","延边州","敦化","吉林三三零五机械厂"," "," "," ","HJD-82B型增雨防雹火箭弹烟剂研制预算150万  \n针对现播撒烟剂燃烧不稳定问题，设计开发适合HJD-82B型增雨防雹火箭弹的播撒烟剂，完成烟剂配方研制，并形成烟剂制备工艺。实现烟剂燃烧可靠、稳定，使点燃过程中及燃烧播撒过程中无爆燃现象，燃烧时  间符合要求。烟剂内含碘化银，是形成增雨防雹晶核载体，是降雨及消、减雹灾作用的主要功能部件。要求适配于HJD-82B型增雨防雹火箭弹系统，催化燃烧时间19s～26s；催化成核率:(试验室内，-10℃条件下)≥1013个每克；烟剂燃烧稳定，不发生爆炸。",2023," "," "," "]
[" "," ",181,"生物医药及先进医疗器械","生物医药医疗","长春","朝阳区","长春西诺生物科技有限公司"," "," "," ","新型疫苗佐剂、口服疫苗/抗体递送系统、活性检测报告基因系统  (1)新型疫苗佐剂：目前国内外获批生物制品所用佐剂基本为自有专  利产品，难以授权使用，且在灭活疫苗产品开发中，由于佐剂诱导的先天性免疫应答不确实，导致针对一些特殊病原的免疫效果不好，急需开发一种免疫增强作用明显且低毒性的佐剂；  (2)口服疫苗/抗体递送系统：口服类疫苗/抗体发挥效应部位在动物体的肠道，但消化道复杂环境因素难以保证疫苗/抗体的活性及驻留释放，需要通过专门的递送系统以保证制品的靶向性、稳定性；  (3)活性检测报告基因系统：基因工程抗体药物的开发需要体外效力  评价系统，目前基本采用重组报告基因细胞的方法，但国内外尚未建立有关宠物相关疾病的报告细胞。",2023," "," "," "]
[" "," ",182,"生物医药及先进医疗器械","生物医药医疗","长春","农安县","吉林恒星科技制药有限公司"," "," "," ","固体制剂工艺技术（预算10万元）  \n内容：①对红花籽油(原油)精制过程中各工艺条件及参数进行确定和验证，并对精制红花油质量控制方法进行分析验证，从而对精制红花油质量进行提升。②对心脑清软胶囊制剂工艺进行优化，③产品质量标准提升。在心脑清软胶囊原质量标准基础上进行提高，增加主要成分维生素B6含量测定项及含量均匀度考察。难点：溶胶工艺进行改进，在原工艺基础上缩短溶胶时间，并且溶胶后胶液质量得到提高，使制得成品弹性好，解决久置粘连问题。",2023," "," "," "]
[" "," ",183,"生物医药及先进医疗器械","生物医药医疗","白城","洮南","吉林康庄大道农业发展有限公司"," "," "," ","杂交玉米制种高产栽培技术（预算2亿元）  \n1、杂交玉米制种高产栽培技术研究；  \n2、高标准种子加工技术研究；  \n3、玉米新品种研发创新。",2023," "," "," "]
[" "," ",184,"生物医药及先进医疗器械","生物医药医疗","长春","农安县","吉林省中亿医药包装有限公司"," "," "," ","增加材料稳定性。",2023," "," "," "]
[" "," ",185,"其他","轻工纺织","白城","洮南","洮南恒盛毛纺织有限公司"," "," "," ","企业产品品质提升，目标：欧洲品质",2023," "," "," "]
[" "," ",186,"汽车电子及新型汽车零部件","汽车及零部件","长春","公主岭市","公主岭轴承有限责任公司"," "," "," ","联合开展一汽康迈结构轮毂单元研发（预算500万元）  \n联合开展康迈结构轮毂单元深层次研发，开展康迈结构轮毂单元轮毂、隔套材质、隔套受力变形对游隙的影响曲线、各组件的互换性等领域研究，开展对材料性能等技术难题的探讨。开展康迈结构轮毂单元试验形式和试验标准研究。",2023," "," "," "]
[" "," ",187,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春新金仑汽车零部件有限公司"," "," "," ","汽车差速器总成设计、仿真及验证（预算500万元）  \n1、汽车差速器总成设计，行星齿轮理论安装距、行星轴孔径的计算，直齿锥齿轮参数设计计算。相关差速器齿轮现有市场的情况。  \n2、差速器总成运行及装配仿真模拟。  \n3、差速器总成性能试验及验证。  \n4、差速器壳体材料轻量化的研究。",2023," "," "," "]
[" "," ",188,"汽车电子及新型汽车零部件","汽车及零部件","吉林","吉林","一汽吉林汽车有限公司"," "," "," ","我公司目前在研产品森雅鸿鹄（R9）是在原燃油车基础上，全面升级新能源的产品项目，该车型具有超长续航（综合续航里程超1100KM）、超强动力（0-50km/h加速2.9s，0-100km/h加速8.4s）、超低油耗（满电油耗1.1L/100KM,亏电油耗4.4L/100KM）及全地域、全季候等特点，且平台可兼容纯电、混动、增程多技术路线，是我公司全新能源转型进程中的关键产品。目前该项目正处于整车标定及试验验证阶段，该产品项目主要涉及通用化新能源平台、智能网联技术、寒区新能源适应性等重点领域，需要产品开发、整车试制、匹配标定、实验验证等方面的支持  ",2023," "," "," "]
[" "," ",189,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春近江汽车零部件有限公司"," "," "," ","1、产品尺寸在线三维影像自动检测技术应用。  \n2、管件内高压成型工艺模拟分析及模具结构设计优化。  \n3、激光焊接制管焊道质量视频监控及自动调整技术应用。",2023," "," "," "]
[" "," ",190,"汽车电子及新型汽车零部件","汽车及零部件","长春","南关区","长春富维伟世通汽车电子有限公司"," "," "," ","1.车载安卓系统应用程序apk开发；  \n2.车载信息娱乐系统人机界面（UI）开发设计；  \n3.Linux系统底层驱动程序BSP开发；  \n4.车载安卓系统中间件（Framework/HAL）开发；  \n5.汽车座舱电子控制器架构设计；",2023," "," "," "]
[" "," ",191,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春一汽富晟李尔汽车电器有限公司"," "," "," ","客户定制开发，主要是研发及生产人员需求",2023," "," "," "]
[" "," ",192,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","博世汽车部件（长春）有限公司"," "," "," ","系统仿真（热管理系统，电磁，电机控制，电机结构，传动系统）；  \n电机控制器控制软硬件开发（座椅，雨刮，举窗电机，电子水泵，其他车用小型无刷电机控制器）；",2023," "," "," "]
[" "," ",{"$f":"ROW()-2","v":193},"汽车电子及新型汽车零部件","汽车及零部件","长春","南关区","长春旭阳工业（集团）股份有限公司"," "," "," ","1、在座椅骨架生产加工过程中主要采用激光焊接工艺，生产过程中焊缝凹陷大的缺陷长期无法解决，具体描述为激光焊缝的收弧部分始终存在凹坑，其深度操过技术标准要求的40%的板材最小板厚，影响焊接强度，请给予此方面技术支持。  \n2、生产制造方面，靠背的调角器核心件为进口零部件，受国外条件制约较大，希望能够在国产化方面能够提供相关资源及技术方面的支持  \n3、用于汽车软内饰产品的新型环保材料及其加工工艺，以及新型高效节能降耗加工设备和工艺解决方案的支持。  \n4、CAE和FEA分析技术；汽车座椅整椅设计技术；汽车座椅护面产品开发技术；汽车座椅泡沫发泡技术等相关技术支持。  汽车内饰注塑模具、表皮包覆模具等和工业自动化的应用集成供应商对接。",2023," "," "," "]
[" "," ",194,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春丽明科技开发股份有限公司"," "," "," ","技术方面：1.智能制造、自动化加工线开发技术  \n2.新能源车辆电子电器开发技术  \n3.车身网络通信信息安全技术  \n4.车辆智能网联开发技术       \n人才方面：1.自动化电气设计开发人才  \n2.自动化机械设计开发人才  \n电子电器设计开发人才",2023," "," "," "]
[" "," ",195,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","兰德（吉林省）科创产业化集团有限公司"," "," "," ","光学光电子、汽车电控零部件相关技术、工业自动化领域伺服控制器相关技术",2023," "," "," "]
[" "," ",196,"汽车电子及新型汽车零部件","汽车及零部件","长春","公主岭市","公主岭华翔汽车顶棚系统有限公司"," "," "," ","有效降低产品VOC（有毒有害挥发性有机物）含量。  \n悬浮式顶棚投影巨幕项目：  \n1、顶棚内置幕布/投影器结构设计；  \n2、幕布收卷结构及控制单元；  \n3、投影器控制单元；  \n4、幕布隔离紫外线功能开发。",2023," "," "," "]
[" "," ",197,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春鸿德汽车照明有限公司"," "," "," ","1、带LIN通信功能的氛围灯通过车身总线控制，实现更加丰富的功能，如颜色变化、亮度调整等，整车厂对带LIN通信功能的氛围灯需求日益增加。LIN通信开发分为硬件和软件，硬件包括器件选型、线路板设计等，软件的程序开发难度较大，首先要获得整车厂LIN协议等要相关输入，开发过程中多次参与整车LIN通信测试。企业投入的LIN通信检测设备和功能检测设备需要从国外引进。  \n车用投影灯受装车空间和出光角度限制，为满足亮度均匀、成像图案晰，设计分析周期较长，为验证设计是否符合要求，现在的做法是通过快速模具的加工样件验证。影响企业在车用投影灯市场的发展速度和竞争力。",2023," "," "," "]
[" "," ",198,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春一汽富维东阳汽车塑料零部件有限公司"," "," "," ","为扩大技术落地规模和不断的升级迭代，在产品设计研发、实验验证、研究性设备投资和技术落地等方面的人力、资金及其相关资源等方面需要支持。",2023," "," "," "]
[" "," ",199,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春富晟汽车饰件有限公司"," "," "," ","资金补助或支持",2023," "," "," "]
[" "," ",200,"汽车电子及新型汽车零部件","汽车及零部件","长春","绿园区","富奥威泰克汽车底盘系统有限公司"," "," "," ","     1.关于专业技术人才是否有专项资金奖励，政策上是否有人才引进扶持；  2.公司研发投入金额高，是否有研发补助相关政策；  3.希望可以多参加汽车技术研讨会，相关技术交流活动。",2023," "," "," "]
[" "," ",201,"汽车电子及新型汽车零部件","汽车及零部件","长春","南关区","长春佛吉亚旭阳汽车座椅有限公司"," "," "," ","  技术瓶颈：我司靠背骨架主要采用激光焊接工艺，生产过程中焊缝凹陷大的缺陷长期无法解决，具体描述为激光焊缝的收弧部分始终存在凹坑，其深度操过技术标准要求的40%的板材最小板厚，影响焊接强度，此问题希望能够得到政府和院校的支持和帮助，或者共同搭建学研合作平台解决。  在生产制造方面，靠背的调角器核心件为进口零部件，受国外条件制约较大，希望能够在国产化方面能够提供相关资源及技术方面的支持。",2023," "," "," "]
[" "," ",202,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春市高新东卓汽车电子有限公司"," "," "," ","  1.自动化产线设计  2.智能工厂规划  3.先进电子技术  4.汽车电子技术       需求相关技能人才",2023," "," "," "]
[" "," ",203,"汽车电子及新型汽车零部件","汽车及零部件","长春","绿园区","长春市汽车冲压件有限公司"," "," "," ","  1、激光焊接技术  2、摩擦焊技术  3、PR铆接技术  4.热成型技术       焊接变形分析软件应用",2023," "," "," "]
[" "," ",204,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春富维汽车视镜系统有限公司"," "," "," ","  CMS电子后视镜",2023," "," "," "]
[" "," ",205,"汽车电子及新型汽车零部件","汽车及零部件","长春","南关区","吉林省通用机械（集团）有限责任公司"," "," "," ","  1.铝铸造技术  2.铝锻造技术  3.冲压技术     铸造工程师、锻造工程师、冲压工程师、CAE工程师、DMU工程师",2023," "," "," "]
[" "," ",206,"汽车电子及新型汽车零部件","汽车及零部件","长春","绿园区","富奥汽车零部件股份有限公司"," "," "," ","  1、铝铸造底盘部件开发技术  2、汽车热泵空调系统开发技术  3、三合一电驱系统产品设计技术  4、汽车全主动悬架系统开发技术  5、线控转向系统开发技术",2023," "," "," "]
[" "," ",207,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春富晟安创汽车零部件有限公司"," "," "," ","  光学、塑料电镀、涂装技术",2023," "," "," "]
[" "," ",208,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","东北工业集团  长春一东离合器股份有限公司"," "," "," ","车载电动无油空气压缩机技术-预算30万  目前车载电动无油空气压缩机是电动商用车空压机发展方向之一。该技术主要解决有油空气压缩机机油乳化、排气压力低、可靠性差等问题。该压缩机需要电机与无油空气压缩机集成技术，由于没有机油润滑，该技术需要解决摩擦材料耐磨性问题，寿命需达到3000小时，噪音需要小于72分贝，并需要与冷却系统集成。",2023," "," "," "]
[" "," ",209,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","东北工业集团  吉林东光奥威汽车制动系统有限公司"," "," "," ","军车制动器试验验证技术-预算5万  军车制动器综合性能试验技术功能要求：安全可靠，制动器产品液压密封性、拖滞力矩、制动力等性能满足相关国家标准要求；  军车制动器疲劳耐久试验技术功能要求：安全可靠，制动器产品高低温静态工作耐久、动态工作耐久、疲劳强度等性能满足相关国家标准要求。",2023," "," "," "]
[" "," ",210,"汽车电子及新型汽车零部件","汽车及零部件","白城","白城","东北工业集团  白城中一精锻股份有限公司"," "," "," ","空心轴锻造技术-预算10万  \n空心轴在传统汽车和新能源汽车上都有广泛应用，如汽车半轴、变速器输入轴、差速器输入轴、齿轮轴、新能源电机传动轴、驱动轴、转向管柱、横向稳定杆等管类锻造件都是利用旋锻技术加工而成。",2023," "," "," "]
[" "," ",211,"汽车电子及新型汽车零部件","汽车及零部件","吉林","吉林","吉林北方捷凯传动轴有限公司"," "," "," ","路谱信号处理及端节选型软件-预算50万  目前主要通过路谱信号来选择驱动轴节型，计算驱动轴总成强度及耐久寿命，因此需要针对路谱信号的处理方法，即雨流计算。  以往的端节选型均为excel编写公式，数据不明朗，操作不方便，因此需要端节选型编制计算程序。",2023," "," "," "]
[" "," ",212,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春众升科技发展有限公司"," "," "," ","1、智能化激光打磨技术。  针对橡胶及塑料等软性材料自适应打磨或者切削。  \n2、智能腔体密封漏点检测技术。针对空腔体的气密性检测，需要检查出具体漏点位置及尺寸，自动完成并能反馈出图像示意；  \n3、特殊密封圈物料分拣及特征识别，缺陷查找并能自动压入对应密封槽内",2023," "," "," "]
[" "," ",213,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","吉林大华机械制造有限公司"," "," "," ","车载高清环视系统(AVM)算法：预算100万元  车载高清环视系统(AVM)算法应用场景是指在汽车行驶或泊车时，通过安装在车身的前、后、左、右四个视觉传感器相互协同配合，进行视频拼接合成处理，呈现行车车身周围360度的视觉图像效果，让驾驶员视野更开阔，消除驾驶员视野盲区，提升驾乘安全性。",2023," "," "," "]
[" "," ",214,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春华翔汽车金属部件有限公司"," "," "," ","1、汽车轻量化金属材料应用；  \n2、节能环保材料应用（汽车金属产品）；  \n3、铝合金免热处理一体化压铸技术应用；  \n4、线控制动、主动悬架系统等机电一体化技术；  \n5、高校有关汽车学院、材料学院、机械学院等方面新技术、新工艺推广应用。",2023," "," "," "]
[" "," ",215,"汽车电子及新型汽车零部件","汽车及零部件","长春","宽城区","长春泰盟机械制造股份有限公司"," "," "," ","制动盘表面防腐处理技术（预算100万元）  主要研究制动盘表面特殊处理技术，以实现无需涂层即可实现防腐能力。制动盘不进行涂层处理即可实现96h盐雾试验能力，提升制动盘防腐能力",2023," "," "," "]
[" "," ",216,"汽车电子及新型汽车零部件","汽车及零部件","长春","朝阳区","长春市长瑞汽车冲压件有限公司"," "," "," ","无痕焊技术指导（预算0.3万元）  \n薄厚板无痕焊接，无痕效果不好，熔深达不到要求，偏核",2023," "," "," "]
[" "," ",217,"汽车电子及新型汽车零部件","汽车及零部件","长春","绿园区","长春市博明汽车部件有限责任公司"," "," "," ","技术攻关内容-发泡线束：  随着汽车工业的发展，人们对汽车的外观、舒适性、安全性、节能性等要求的不断提高，塑料制品在汽车零部件上的用量也在不断的提高。利用发泡技术代替传统的护板及支架不仅可以减轻线束重量而且还便于线束的空间布置。由聚氨酯制成的线束（发泡线束）具有重量轻、抗油污、粉尘能力强，安装后没有噪声等特点。  \n难点：目前发泡线束只在在设计基本型产品固化和结构复杂的干线区域采用发泡，我公司发动机线束目前还没有应用发泡线束，\n原因如下：1、发泡材料不耐高温，发动机线束的使用环境一般在-40℃～+125℃，使用的高温区甚至接近200℃  \n2、发泡材料是一次成型，要求在产品固化的位置应用，但商用车、非道路柴油机线束的特点就是品种多、产品批量小、变型多且频繁、交付周期短、订单变化快  目前紧局限于特殊需求特殊部位采用，在常规线束上并未采用。",2023," "," "," "]
[" "," ",218,"汽车电子及新型汽车零部件","汽车及零部件","长春","公主岭市","吉林瀚腾汽车部件（集团）有限公司"," "," "," ","主动安全式前盖铰链研发（预算200万元）  \n目前随着汽车设计更注重行人保护，对于主动安全式前盖铰链的需求成为新的发展方向。  \n难点：主动式前盖铰链结构、功能及设计。",2023," "," "," "]
[" "," ",219,"汽车电子及新型汽车零部件","汽车及零部件","长春","公主岭市","吉林省红星轨道车辆装备有限公司"," "," "," ","模具开发设计、新材料研发替代。",2023," "," "," "]
[" "," ",220,"汽车电子及新型汽车零部件","汽车及零部件","长春","二道区","长春汽车滤清器有限责任公司"," "," "," ","分析类软件版权费用问题（预算200万元）  一些分析软件购买投入大，分析类工程师人员少，成本高，企业自行培养相关人才后流失率高。企业可自行进行分析，提供报告给客户。",2023," "," "," "]
[" "," ",221,"其他","公共事业","长春","南关区","吉林同鑫热力集团有限公司"," "," "," ","预算500万元  新型蓄能材料的研发、蓄能效率的提高。",2023," "," "," "]
[" "," ",222,"其他","建筑建材","长春","榆树市","长春实德节能建材有限公司"," "," "," ","资金需求：配方调试（预算10万元）",2023," "," "," "]
[" "," ",223,"光电子及智能传感器","电子信息","长春","绿园区","长春昆仑建设股份有限公司"," "," "," ","衍生式多重性能设计驱动的建筑机器人关键技术应用研究（预算60万）  1、如何在装饰装修项目中以衍生式多重性能驱动式设计作为数字化设计手段；  2、如何基于衍生式多重性能驱动式设计，将装饰装修的建筑机器人应用于施工过程中。",2023," "," "," "]
[" "," ",224,"光电子及智能传感器","电子信息","长春","宽城区","吉林省差旅天下网络技术股份有限公司"," "," "," ","面向企业级消费数智化费用控制管理的AI人工智能（区块链技术、物联网技术、大数据算法）应用软件开发技术开发服务需求等  自动驾驶、车路协同技术  主要解决自动驾驶关于物流倒运方面的技术难点，其中涉及到车路协同、离地倒运、正装正卸等技术",2023," "," "," "]
[" "," ",225,"光电子及智能传感器","电子信息","长春","绿园区","一汽物流有限公司"," "," "," ","自动驾驶、车路协同技术",2023," "," "," "]
[" "," ",226,"光电子及智能传感器","电子信息","长春","朝阳区","吉林省燚盟科技股份有限公司"," "," "," ","相关前端传感器的研发、算法技术提升等：预算260万元  智慧水务传感器研发，可信数据传输，大规模数字孪生场景建设，高精度数据底板构建，算法平台建设，以实现事件推演和预警。  \n一、技术参数：  \n1、在智慧水务系统中对管道，防汛抗灾，水资源监控，给排水等应用场景实现全量数据实时采集和管理联动。  \n2、进行城市水资源管理数字孪生技术研究，满足实时监测，仿真模拟，智能推演，自动控制等功能。  \n二、相关指标描述：  \n1、实现50平方公里以上大区域GIS数据采集和动态更新。  \n2、流量、流速采样偏差小于1%。  \n3、百万级前端数据可靠传输，响应时间小于1s。",2023," "," "," "]
[" "," ",227,"光电子及智能传感器","电子信息","长春","绿园区","富赛汽车电子有限公司"," "," "," ","自动驾驶感知融合与车辆规划控制技术（预算5000万元）  \n高阶L2+以上的自动驾驶域控制器，需要融合前视，周视摄像头，毫米波雷达，激光雷达，V2X超视距等传感器的感知数据进行融合，构建电子地图，形成行车空间，并控制车辆按照设定的路径行进；在此过程中，可部署到嵌入式系统之上的多传感器感知融合算法，路径规划算法，车辆规控算法等技术成为自动驾驶的关键技术。",2023," "," "," "]
[" "," ",228,"光电子及智能传感器","电子信息","长春","朝阳区","长春艾希技术有限公司"," "," "," ","汽车视觉引导自动装配技术研究：视觉引导方向的四个难点：第一，当前双目的三维检测精度基本都在一毫米以上，这个精度比较低，对于抓取和定位，不太容易实现；第二，3D轮廓检测微小的轮廓检测精度是挺高的，但是适用范围比较小，一般在加减20毫米左右，这种对于有些定位场合，显得这个视觉范围太小，而且都主要集中在一些技术基础产品，国产的产品可能进度还不如这个。第三、是视觉的传输速度问题，就是经过拍照定位计算，如果要实时传输给PLC或者电气系统，它这个传输速度比较慢，如果用它来做视觉引导，就是同步运动的话，可能会有问题。第四、是个通用的问题，就是现在的视频对环境光源影响比较大，在白天，黑天，阴天晴天，或者现场开灯没开灯，影响比较大，这个比较难解决。\n汽车涂胶泵和定量机齿轮泵的研发：\n（1）汽车自动涂胶站中的涂胶泵研发：在做汽车生产线的涂胶站过程中，我们通常用的国外的涂胶泵的参数是单冲程165ccm冲胶量（焊装用胶泵）；单冲程301ccm出胶量（总装用胶泵）。如果涂胶泵能自己研发成功，可以替代进口产品；\n（2）汽车自动涂胶站中的定量机齿轮泵研发。定量机齿轮泵是汽车涂胶过程中的计量系统，关键参数涉及伺服电机转多少转涂胶量及齿轮啮合出胶量。  \n（3）其中密封件的参数和设计情况也是重点。   ",2023," "," "," "]
[" "," ",229,"光电子及智能传感器","电子信息","长春","朝阳区","东北工业集团有限公司"," "," "," ","1、电液智能助力器（IEHB）控制系统技术；  \n2、整车控制系统技术（VCU）；  \n3、激光雷达信息处理技术；  \n4、图像传感器和图像处理技术；  \n5、多传感器融合算法技术。",2023," "," "," "]
[" "," ",230,"光电子及智能传感器","电子信息","长春","朝阳区","长春一东离合器股份有限公司"," "," "," ","  1.激光雷达产品设计技术，激光雷达发射系统激光器设计开发技术，接收系统光电探测器设计开发技术，信息处理系统FPGA芯片、模拟芯片设计技术；  2.激光雷达产品测试、试验验证技术及资源。       1.与吉林大学、长春理工大学产学对激光雷达应用软件算法产学研开发，培养本地技术人才；  2.与长光卫星、光机所等企业合作，共建激光雷达产业链；  3.激光雷达产品高端领军人才引入；  4.激光雷达产品项目开发资金、税收方面的支持。",2023," "," "," "]
[" "," ",231,"光电子及智能传感器","电子信息","长春","朝阳区","长春吉大正元信息技术股份有限公司"," "," "," ","基于零信任的动态自适应权限策略管理与访问控制-预算650万  面向X场景信息系统资源细粒度管控需求，研究基于流量自学习的权限策略综合治理、面向X场景云环境的微隔离控制、面向X场景大数据平台的细粒度访问控制、面向API的智能访问控制等关键技术，基于特定任务要求、信任评估结果等因素，实现权限策略综合治理、自适应调整和智能协同访问控制，支撑构建覆盖“用户-终端-网络-应用-服务-数据”全业务访问周期的动态访问控制机制。",2023," "," "," "]
[" "," ",232,"光电子及智能传感器","电子信息","长春","朝阳区","长春启璞科技信息咨询有限公司"," "," "," ","解决工业软件和工业APP在云中数据的流动、存储、使用的数据信息安全问题：预算100万元  需解决的主要技术难题：随着公有云、私有云、混合云的蓬勃发展，越来越多的企业将的重要业务系统都在迁入云中，上云上平台后，如何解决云中数据的流动、存储、使用的数据信息安全问题也成为了困扰启璞云端业务开展的核心诉求。",2023," "," "," "]
[" "," ",233,"光电子及智能传感器","电子信息","长春","朝阳区","长春博瑞达光电子有限公司"," "," "," ","预算2万元  \n不同材料的工艺不同，材料磨削度不同，采用不同的工艺加工。微透镜的粗糙度控制，内窥镜镜头的设计和测试",2023," "," "," "]
[" "," ",234,"精密仪器及先进装备","新材料","吉林","永吉","吉林省固和泰机械有限责任公司"," "," "," ","新型快充锂离子电池  \n锂离子电池；电池容量：54Ah；电池电压：12V  \n工作温度：放电-20度到65度，充电0-55度。  \n大容量锂电池组，充放电500次以上。",2023," "," "," "]
[" "," ",235,"人工智能机智能机器人","人工智能","长春","汽开区","无界融合（吉林）科技有限公司","白光 线光谱及点光谱测量仪产品","无界融合（吉林）科技有限公司成立于2023年01月28日，注册地位于长春市汽车开发区兴顺路1366号9009、9010室，法定代表人为赵岩。经营范围包括一般项目：软件开发；软件销售；软件外包服务；人工智能应用软件开发；人工智能基础软件开发；人工智能理论与算法软件开发；信息技术咨询服务；电子专用材料销售；电子专用材料研发；5G通信技术服务；信息系统运行维护服务；数字技术服务；工业互联网数据服务。（除依法须经批准的项目外，凭营业执照依法自主开展经营活动）"," ","1、白光线光谱及点光谱测量仪——测量透明/半透明产品的厚度或者移动测量产品相对  位置信息等数据；  \n2、光学分光方式：干涉或者共焦方式都可以；  3、对应点或线的 CMOS/CCD 传感器接收。  ",2023,11,"李佳錞",18686600072]
[" "," ",236,"光电子及智能传感器","电子器件","长春","新区","长春维鸿东光电子器材有限公司","高介电常数薄膜研发","公司现为“国家级高新技术企业”、“吉林省专精特新企业”、“长春市科技小巨人企业”。公司坐落于长春市高新技术产业开发区，占地面积1.25万平方米，资产总额为1.5亿元，公司现有员工220余人，高级工程师40余人，中级工程师50余人。","公司目前电容器常用薄膜的介电常数普遍为3左右或者更低，急需介电常数更高的薄膜，用于缩减产品体积，满足用户整机小型化要求。","高介电常数薄膜20㎡。  \n电子元器件市场所需产品已向小体积，高容量，耐高温方向发展，为研制介电常数达到10左右，可将电容器体积缩减为原来的三分之一的产品，高介电常数薄膜。",2023,11,"徐志刚","0431-88010030"]
[" "," ",237,"其他","环境科学与工程类","长春","新区","长春永固科技有限公司","高污染物浓度废液处理工艺与乙醇回收工艺的研究及车间设计","长春永固科技有限公司成立于2007年，致力于芯片粘接胶水的研发、生产、销售。公司被认定为高新技术企业、国家专精特新“小巨人”企业、吉林省“专精特新”中小企业、吉林省科技小巨人企业、、吉林省省级企业技术中心、长春市“专精特新”中小企业、长春市科技小巨人企业、长春市市级企业技术中心。","公司在银粉国国产化方面，投入研发力量，致力于解决依赖银粉进口，技术卡脖子难题。但在银粉的生产中所产生的废液，目前无法达到环保排放要求，成为了银粉国产化项目的主要阻碍。因此需要突破废水处理工艺研究、乙醇回收工艺的研究、废液处理工艺与乙醇回收工艺车间的设计。  技术难题：  1.高污染物浓度废液处理工艺的研究；  2.废液中乙醇回收工艺的研究；  3.废液处理工艺与乙醇回收工艺车间的设计。","处理方案一套。\n技术标准：  \n1.日处理量3t；  \n2.将废液中的乙醇回收成无水乙醇；  \n3.废液分三种：高污染物浓度水;中等污染物浓度水和乙醇的溶液;低污染物浓度乙醇。  \n4.上述废液的混污染物含量如下：COD约105-106mg/L; 氨氮约103-104mg/L;总有机碳约105-106mg/L；总氮约103-104",2023,11,"王彩霞","13756010344"]
[" "," ",238,"生物医药及先进医疗器械","材料类","长春","九台","吉林省沃鸿医疗器械制造有限公司","硅橡胶材料改性研发","公司总部位于长春市南关区新星宇商誉，办公面积近600平方米，生产场地位于长春九台经济开发区卡伦工业北区甲三路16号。占地面积7000余平方米，场地属自主产权，建筑面积约5000平方米，拥有10万级净化车间三座，面积约2000平方米。公司现有从业人员91人，其中管理人员及技术人员23人，均为大专以上学历，其中高级技术职称5人，中级技术职称2人，公司研发中心技术力量雄厚，拥有完善的科研、生产、质量检测。","骨科肢体手术最理想的方法是先驱除肢体的血液然后阻断肢体的动脉血管，这样才能才能使手术视野清晰，不会引起术中出血。目前国内采取的都是套扎的方式，没有驱血的功能，这样会导致静脉血液的流失，而且止血效果不是很理想。而我公司正在研究一款具有驱血止血的器械，来解决临床手术中驱血止血不彻底的难题！","交付一套成熟的加工方案及材料配比。本产品计划用硅胶材质做成圆形套环，利用硅胶材质的弹性来驱赶肢体血液的并阻断动脉血的流动，需要解决的是利用不同直径，不同硬度的硅胶来应对不同人群肢体差异的问题，而且材质需要极高的稳定性。",2023,11,"许凯","15092859675"]
[" "," ",239,"生物基新材料","材料类","长春","绿园","长春市城建维护集团股份有限公司","土壤（污泥）固结及资源化利用技术研发","长春市城建维护集团股份有限公司，成立于1998年9月17日，股份制企业，注册资本2亿元，是中庆集团旗下控股子公司，致力于成为中国一流城市基础设施运营服务商。城建维护集团深耕基础设施维护运营与基础设施建设两大业务板块，在道路桥梁、轨道交通、园林绿化、生态环保、智慧环卫等领域，为客户提供全方位服务和系统化解决方案。","(1)土壤固化剂配合比  (2)土壤固化剂掺量对固化土力学性能的影响  (3)土壤固化剂稳定土耐久性能  (4)废弃土方固化土强度形成机理研究","样品和技术研究报告1份。  \n(1)制备一种土壤固化剂，10h强度达到0.3-30MPa，抗渗3-5bar。  \n(2)获得土壤固化剂最佳掺量，推迟施工8h，仍满足石灰稳定材料各等级公路路基底基层的强度要求（＞0.8MPa）。",2023,11,"李经理","18686518721"]
[" "," ",240,"碳纤维及复合材料","材料类","长春","宽城","吉林省新奇建筑电气有限公司","太阳能玻璃模块研发","本企业是集科研开发、制造、经营的体制。主要产品：加工生产箱式变电站，各种高、低压配电屏，动力、照明配电箱，计量箱，供水成套设备，工业自动化仪表盘、操作台，电锅炉配电屏，电缆桥架，母线槽，不锈钢制品，玻璃钢制品，太阳能制品，永磁耦合热源电采暖炉，小型风力发电机，热储能设备、翻转式电脑桌和翻转式电脑操作台等多项实用新型专利证书的新产品，并获得电气产品CCC强制性认证。","解决建筑用太阳能玻璃罩及底壳连接密封性不好，底壳用材料在安装过程中安全性差的问题。","太阳能玻璃及底壳一体化设计方案一套。  \n太阳能玻璃罩及底壳一体化设计，确定底壳用材料，实现太阳能发电及产热，达到真空、保温、抗震、防火，确保恶劣自然条件下安全性。",2023,11,"袁进","13944127558"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "]